<?xml version="1.0" encoding="UTF-8" ?>
<DelphinProject xmlns="http://www.bauklimatik-dresden.de" xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xmlns:IBK="http://www.bauklimatik-dresden.de/IBK" xsi:schemaLocation="http://www.bauklimatik-dresden.de DelphinProject.xsd" fileVersion="6.4">
	<ProjectInfo created="Tue Mar 10 16:38:16 2009" lastEdited="Di. Sep. 26 07:27:28 2017">
		<Comment>&lt;p style=&quot; margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;&quot;&gt;&lt;span style=&quot; font-family:&apos;Courier&apos;; font-weight:600;&quot;&gt;DIN EN ISO 10211 - Case 1&lt;/span&gt;&lt;/p&gt;&#x0A;&lt;p style=&quot;-qt-paragraph-type:empty; margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px; font-family:&apos;Courier&apos;;&quot;&gt;&lt;br /&gt;&lt;/p&gt;&#x0A;&lt;p style=&quot; margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;&quot;&gt;&lt;span style=&quot; font-family:&apos;Courier&apos;;&quot;&gt;A simple rectangular 2D calculation, where correct application of boundary conditions is tested. &lt;/span&gt;&lt;/p&gt;&#x0A;&lt;p style=&quot;-qt-paragraph-type:empty; margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px; font-family:&apos;Courier&apos;;&quot;&gt;&lt;br /&gt;&lt;/p&gt;&#x0A;&lt;p style=&quot; margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;&quot;&gt;&lt;span style=&quot; font-family:&apos;Courier&apos;;&quot;&gt;The example illustrates the use of two material references to the same material file that allow the automatic grid generation algorithm to cluster near the points of interest.&lt;/span&gt;&lt;/p&gt;&#x0A;&lt;p style=&quot;-qt-paragraph-type:empty; margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px; font-family:&apos;Courier&apos;;&quot;&gt;&lt;br /&gt;&lt;/p&gt;&#x0A;&lt;p style=&quot; margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;&quot;&gt;&lt;span style=&quot; font-family:&apos;Courier&apos;;&quot;&gt;The numerical parameters in this example are tuned for steady-state thermal calculation: KLU sparse direct equation solver, strict Newton tolerances, but loose time integration tolerances.&lt;/span&gt;&lt;/p&gt;&#x0A;&lt;p style=&quot; margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;&quot;&gt;&lt;span style=&quot; font-family:&apos;Courier&apos;;&quot;&gt; &lt;/span&gt;&lt;/p&gt;</Comment>
	</ProjectInfo>

	<!--~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~-->

	<!--Model data, solver settings, general parameters-->
	<Init>
		<SimulationParameter>
			<BalanceEquationModule>BEHeat</BalanceEquationModule>
			<Interval>
				<IBK:Parameter name="Duration" unit="d">40</IBK:Parameter>
			</Interval>
			<LambdaSelection>LambdaDry</LambdaSelection>
		</SimulationParameter>
		<SolverParameter>
			<Integrator>CVODE</Integrator>
			<LESSolver>KLU</LESSolver>
			<IBK:Parameter name="MaxTimeStep" unit="d">1</IBK:Parameter>
			<IBK:Parameter name="MinTimeStep" unit="s">1e-05</IBK:Parameter>
			<IBK:Parameter name="InitialTimeStep" unit="s">100</IBK:Parameter>
			<IBK:Parameter name="RelTol" unit="---">0.1</IBK:Parameter>
			<IBK:Parameter name="AbsTolEnergy" unit="---">0.1</IBK:Parameter>
			<IBK:Parameter name="AbsTolMoisture" unit="---">1e-06</IBK:Parameter>
			<IBK:Parameter name="AbsTolAir" unit="---">1e-06</IBK:Parameter>
			<IBK:Parameter name="AbsTolSalt" unit="---">1e-10</IBK:Parameter>
			<IBK:Parameter name="AbsTolPollutant" unit="---">1e-12</IBK:Parameter>
			<IBK:Parameter name="NonlinSolverConvCoeff" unit="---">1e-05</IBK:Parameter>
		</SolverParameter>
	</Init>

	<!--~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~-->

	<!--List of all materials used in this construction-->
	<Materials>
		<MaterialReference name="Concrete_C20_25" color="#ffa909ff">${Project Directory}/materials/Concrete_C20_25_10000.m6</MaterialReference>
		<MaterialReference name="Concrete_C20_25 [2]" color="#ff80ff00">${Project Directory}/materials/Concrete_C20_25[2]_10001.m6</MaterialReference>
	</Materials>

	<!--~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~-->

	<!--Discretization data (grid and sketches)-->
	<Discretization>
		<XSteps unit="m">0.001 0.00143089 0.00204746 0.0029297 0.00419209 0.00599844 0.00858314 0.0122816 0.0175736 0.0197037 0.0197037 0.0197037 0.0197037 0.0197037 0.0197037 0.0197037 0.0175736 0.0122816 0.00858314 0.00599844 0.00419209 0.0029297 0.00204746 0.00143089 0.001 0.001 0.00143089 0.00204746 0.0029297 0.00419209 0.00599844 0.00858314 0.0122816 0.0175736 0.0197037 0.0197037 0.0197037 0.0197037 0.0197037 0.0197037 0.0197037 0.0175736 0.0122816 0.00858314 0.00599844 0.00419209 0.0029297 0.00204746 0.00143089 0.001 0.001 0.00143089 0.00204746 0.0029297 0.00419209 0.00599844 0.00858314 0.0122816 0.0175736 0.0197037 0.0197037 0.0197037 0.0197037 0.0197037 0.0197037 0.0197037 0.0175736 0.0122816 0.00858314 0.00599844 0.00419209 0.0029297 0.00204746 0.00143089 0.001 0.001 0.00143089 0.00204746 0.0029297 0.00419209 0.00599844 0.00858314 0.0122816 0.0175736 0.0197037 0.0197037 0.0197037 0.0197037 0.0197037 0.0197037 0.0197037 0.0175736 0.0122816 0.00858314 0.00599844 0.00419209 0.0029297 0.00204746 0.00143089 0.001 </XSteps>
		<YSteps unit="m">0.001 0.00143089 0.00204746 0.0029297 0.00419209 0.00599844 0.00858314 0.0122816 0.0175736 0.0197037 0.0197037 0.0197037 0.0197037 0.0197037 0.0197037 0.0197037 0.0175736 0.0122816 0.00858314 0.00599844 0.00419209 0.0029297 0.00204746 0.00143089 0.001 0.001 0.00143089 0.00204746 0.0029297 0.00419209 0.00599844 0.00858314 0.0122816 0.0175736 0.0197037 0.0197037 0.0197037 0.0197037 0.0197037 0.0197037 0.0197037 0.0175736 0.0122816 0.00858314 0.00599844 0.00419209 0.0029297 0.00204746 0.00143089 0.001 0.001 0.00143089 0.00204746 0.0029297 0.00419209 0.00599844 0.00858314 0.0122816 0.0175736 0.0197037 0.0197037 0.0197037 0.0197037 0.0197037 0.0197037 0.0197037 0.0175736 0.0122816 0.00858314 0.00599844 0.00419209 0.0029297 0.00204746 0.00143089 0.001 0.001 0.00143089 0.00204746 0.0029297 0.00419209 0.00599844 0.00858314 0.0122816 0.0175736 0.0197037 0.0197037 0.0197037 0.0197037 0.0197037 0.0197037 0.0197037 0.0175736 0.0122816 0.00858314 0.00599844 0.00419209 0.0029297 0.00204746 0.00143089 0.001 0.001 0.00143089 0.00204746 0.0029297 0.00419209 0.00599844 0.00858314 0.0122816 0.0175736 0.0197037 0.0197037 0.0197037 0.0197037 0.0197037 0.0197037 0.0197037 0.0175736 0.0122816 0.00858314 0.00599844 0.00419209 0.0029297 0.00204746 0.00143089 0.001 0.001 0.00143089 0.00204746 0.0029297 0.00419209 0.00599844 0.00858314 0.0122816 0.0175736 0.0197037 0.0197037 0.0197037 0.0197037 0.0197037 0.0197037 0.0197037 0.0175736 0.0122816 0.00858314 0.00599844 0.00419209 0.0029297 0.00204746 0.00143089 0.001 0.001 0.00143089 0.00204746 0.0029297 0.00419209 0.00599844 0.00858314 0.0122816 0.0175736 0.0197037 0.0197037 0.0197037 0.0197037 0.0197037 0.0197037 0.0197037 0.0175736 0.0122816 0.00858314 0.00599844 0.00419209 0.0029297 0.00204746 0.00143089 0.001 0.001 0.00143089 0.00204746 0.0029297 0.00419209 0.00599844 0.00858314 0.0122816 0.0175736 0.0197037 0.0197037 0.0197037 0.0197037 0.0197037 0.0197037 0.0197037 0.0175736 0.0122816 0.00858314 0.00599844 0.00419209 0.0029297 0.00204746 0.00143089 0.001 </YSteps>
	</Discretization>

	<!--~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~-->

	<!--Conditions data, specifies how construction interacts with environment-->
	<Conditions>

		<Interfaces>
			<Interface name="Interface 1" type="Detailed">
				<BCReference>Inside Heat Conduction</BCReference>
			</Interface>
			<Interface name="Interface 2" type="Detailed">
				<BCReference>Outside Heat Conduction</BCReference>
			</Interface>
		</Interfaces>

		<ClimateConditions>

			<ClimateCondition name="Inside Temperature (constant)" type="Temperature" kind="Constant">
				<IBK:Parameter name="ConstantValue" unit="C">20</IBK:Parameter>
			</ClimateCondition>

			<ClimateCondition name="Outside Temperature (constant)" type="Temperature" kind="Constant">
				<IBK:Parameter name="ConstantValue" unit="C">0</IBK:Parameter>
			</ClimateCondition>
		</ClimateConditions>

		<BoundaryConditions>

			<BoundaryCondition name="Inside Heat Conduction" type="HeatConduction" kind="SurfaceValue">
				<CCReference type="Temperature">Inside Temperature (constant)</CCReference>
			</BoundaryCondition>

			<BoundaryCondition name="Outside Heat Conduction" type="HeatConduction" kind="SurfaceValue">
				<CCReference type="Temperature">Outside Temperature (constant)</CCReference>
			</BoundaryCondition>
		</BoundaryConditions>
	</Conditions>

	<!--~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~-->

	<!--Contains definitions of output files and schedules for outputs.-->
	<Outputs>
		<!--General parameters-->
		<IBK:Unit name="TimeUnit">d</IBK:Unit>
		<IBK:Flag name="BinaryFormat">false</IBK:Flag>
		<!--List of all Output schedules-->
		<OutputGrids>
			<OutputGrid name="Profiles">
				<Interval>
					<IBK:Parameter name="Duration" unit="d">0</IBK:Parameter>
					<IBK:Parameter name="StepSize" unit="d">5</IBK:Parameter>
				</Interval>
			</OutputGrid>
		</OutputGrids>
		<!--List of all Output files-->
		<OutputFiles>
			<OutputFile name="TempField1">
				<Quantity>Temperature</Quantity>
				<TimeType>None</TimeType>
				<SpaceType>Single</SpaceType>
				<OutputGrid>Profiles</OutputGrid>
			</OutputFile>
			<OutputFile name="TempField2">
				<Quantity>Temperature</Quantity>
				<TimeType>None</TimeType>
				<SpaceType>Single</SpaceType>
				<OutputGrid>Profiles</OutputGrid>
			</OutputFile>
			<OutputFile name="TempField3">
				<Quantity>Temperature</Quantity>
				<TimeType>None</TimeType>
				<SpaceType>Single</SpaceType>
				<OutputGrid>Profiles</OutputGrid>
			</OutputFile>
			<OutputFile name="TempField4">
				<Quantity>Temperature</Quantity>
				<TimeType>None</TimeType>
				<SpaceType>Single</SpaceType>
				<OutputGrid>Profiles</OutputGrid>
			</OutputFile>
			<OutputFile name="TempField5">
				<Quantity>Temperature</Quantity>
				<TimeType>None</TimeType>
				<SpaceType>Single</SpaceType>
				<OutputGrid>Profiles</OutputGrid>
			</OutputFile>
			<OutputFile name="TempField6">
				<Quantity>Temperature</Quantity>
				<TimeType>None</TimeType>
				<SpaceType>Single</SpaceType>
				<OutputGrid>Profiles</OutputGrid>
			</OutputFile>
			<OutputFile name="TempField7">
				<Quantity>Temperature</Quantity>
				<TimeType>None</TimeType>
				<SpaceType>Single</SpaceType>
				<OutputGrid>Profiles</OutputGrid>
			</OutputFile>
		</OutputFiles>
	</Outputs>

	<!--~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~-->

	<!--List of all assignments of materials and conditions-->
	<Assignments>

		<Assignment type="Material" location="Element">
			<Reference>Concrete_C20_25</Reference>
			<Range>0 0 99 199</Range>
		</Assignment>

		<Assignment type="Material" location="Element">
			<Reference>Concrete_C20_25 [2]</Reference>
			<Range>25 175 49 199</Range>
		</Assignment>

		<Assignment type="Material" location="Element">
			<Reference>Concrete_C20_25 [2]</Reference>
			<Range>75 175 99 199</Range>
		</Assignment>

		<Assignment type="Material" location="Element">
			<Reference>Concrete_C20_25 [2]</Reference>
			<Range>50 150 74 174</Range>
		</Assignment>

		<Assignment type="Material" location="Element">
			<Reference>Concrete_C20_25 [2]</Reference>
			<Range>0 150 24 174</Range>
		</Assignment>

		<Assignment type="Material" location="Element">
			<Reference>Concrete_C20_25 [2]</Reference>
			<Range>25 125 49 149</Range>
		</Assignment>

		<Assignment type="Material" location="Element">
			<Reference>Concrete_C20_25 [2]</Reference>
			<Range>75 125 99 149</Range>
		</Assignment>

		<Assignment type="Material" location="Element">
			<Reference>Concrete_C20_25 [2]</Reference>
			<Range>0 100 24 124</Range>
		</Assignment>

		<Assignment type="Material" location="Element">
			<Reference>Concrete_C20_25 [2]</Reference>
			<Range>50 100 74 124</Range>
		</Assignment>

		<Assignment type="Material" location="Element">
			<Reference>Concrete_C20_25 [2]</Reference>
			<Range>25 75 49 99</Range>
		</Assignment>

		<Assignment type="Material" location="Element">
			<Reference>Concrete_C20_25 [2]</Reference>
			<Range>75 75 99 99</Range>
		</Assignment>

		<Assignment type="Material" location="Element">
			<Reference>Concrete_C20_25 [2]</Reference>
			<Range>0 50 24 74</Range>
		</Assignment>

		<Assignment type="Material" location="Element">
			<Reference>Concrete_C20_25 [2]</Reference>
			<Range>50 50 74 74</Range>
		</Assignment>

		<Assignment type="Material" location="Element">
			<Reference>Concrete_C20_25 [2]</Reference>
			<Range>25 25 49 49</Range>
		</Assignment>

		<Assignment type="Material" location="Element">
			<Reference>Concrete_C20_25 [2]</Reference>
			<Range>75 25 99 49</Range>
		</Assignment>

		<Assignment type="Material" location="Element">
			<Reference>Concrete_C20_25 [2]</Reference>
			<Range>50 0 74 24</Range>
		</Assignment>

		<Assignment type="Material" location="Element">
			<Reference>Concrete_C20_25 [2]</Reference>
			<Range>0 0 24 24</Range>
		</Assignment>

		<Assignment type="Output" location="Element">
			<Reference>TempField1</Reference>
			<Range>0 175 99 175</Range>
		</Assignment>

		<Assignment type="Output" location="Element">
			<Reference>TempField2</Reference>
			<Range>0 150 99 150</Range>
		</Assignment>

		<Assignment type="Output" location="Element">
			<Reference>TempField3</Reference>
			<Range>0 125 99 125</Range>
		</Assignment>

		<Assignment type="Output" location="Element">
			<Reference>TempField4</Reference>
			<Range>0 100 99 100</Range>
		</Assignment>

		<Assignment type="Output" location="Element">
			<Reference>TempField5</Reference>
			<Range>0 75 99 75</Range>
		</Assignment>

		<Assignment type="Output" location="Element">
			<Reference>TempField6</Reference>
			<Range>0 50 99 50</Range>
		</Assignment>

		<Assignment type="Output" location="Element">
			<Reference>TempField7</Reference>
			<Range>0 25 99 25</Range>
		</Assignment>

		<Assignment type="Interface" location="Top">
			<Reference>Interface 1</Reference>
			<Range>0 199 99 199</Range>
		</Assignment>

		<Assignment type="Interface" location="Left">
			<Reference>Interface 2</Reference>
			<Range>0 0 0 199</Range>
		</Assignment>

		<Assignment type="Interface" location="Bottom">
			<Reference>Interface 2</Reference>
			<Range>0 0 99 0</Range>
		</Assignment>
	</Assignments>

	<!--~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~-->

</DelphinProject>
