[PROJECT_INFO]

  FILE_VERSION             = 5.9.3
  CREATED                  = Tue Jun 06 15:06:58 2017
  LAST_EDIT                = Wed Jan 17 14:43:11 2018


; ******************************************************************************


[INIT]

  [GENERAL]
    BALANCE_EQUATIONS        = ENERGY MOISTURE 
    USE_KIRCHHOFF            = yes
    USE_GRAVITY              = no
    USE_BUOYANCY             = no
    USE_HYDROSTATIC          = no
    PRESSURE_UPDATE_INTERVAL = 10 min
    START_YEAR               = 2017
    START_TIME               = 0
    DURATION                 = 1 a
    ISOTHERMAL_T_REF         = 20 C

  [SALT_SETTINGS]
    USE_EXTRA_SALT_OUTPUT    = no
    USE_OVERSATURATION       = no
    USE_DENSITY              = yes
    FLOW_RESISTANCE_FACTOR   = 0


  [SOLVER_SETTINGS]

    [CVODE_SOLVER_SETTINGS]
      INITIAL_DT               = 0.01 s
      MAX_DT                   = 30 min
      MIN_DT                   = 1e-09 s
      REL_TOL                  = 1e-05
      ABS_TOL_ENERGY           = 0.1
      ABS_TOL_MOISTURE         = 1e-06
      ABS_TOL_AIR              = 1e-06
      ABS_TOL_SALT             = 1e-10
      ABS_TOL_POLLUTANT        = 1e-12
      USE_AUTO_RECOVER         = yes
      MAX_ORDER                = 5
      MAX_STEPS                = 1000000
      USE_MONITORS_FILE        = no
      USE_ONE_STEP_MONITORS    = no
      PREVENT_OVERFILLING      = yes
      USE_STRICT_RANGE_CHECKING = no




; ******************************************************************************


[MATERIALS]

  [MATERIAL]
    EXTERNAL                 = $(PROJECT_DIR)/Materialdaten/Altbauziegel Dresden ZE.m6

    [IDENTIFICATION]
      NAME                     = Altbauziegel Dresden ZE
      COLOUR                   = #ffdb2b60
      UNIQUE_ID                = 0


  [MATERIAL]
    EXTERNAL                 = $(PROJECT_DIR)/Materialdaten/Levelling Plaster.m6

    [IDENTIFICATION]
      NAME                     = Levelling Plaster
      COLOUR                   = #ff00ff00
      UNIQUE_ID                = 0


  [MATERIAL]
    EXTERNAL                 = $(PROJECT_DIR)/Materialdaten/Calsitherm KP Glue Mortar.m6

    [IDENTIFICATION]
      NAME                     = Calsitherm KP Glue Mortar
      COLOUR                   = #ffff00ff
      UNIQUE_ID                = 0


  [MATERIAL]
    EXTERNAL                 = $(PROJECT_DIR)/Materialdaten/Calsitherm Climate Board WF.m6

    [IDENTIFICATION]
      NAME                     = Calsitherm Climate Board WF
      COLOUR                   = #ff8080ff
      UNIQUE_ID                = 0


  [MATERIAL]
    EXTERNAL                 = $(PROJECT_DIR)/Materialdaten/Calsitherm KP Lime Plaster.m6

    [IDENTIFICATION]
      NAME                     = Calsitherm KP Lime Plaster
      COLOUR                   = #ff409020
      UNIQUE_ID                = 0


  [MATERIAL]
    EXTERNAL                 = $(PROJECT_DIR)/Materialdaten/Mineral Wool 035.m6

    [IDENTIFICATION]
      NAME                     = Mineral Wool 035
      COLOUR                   = #fff7fe2e
      UNIQUE_ID                = 0


  [MATERIAL]
    EXTERNAL                 = $(PROJECT_DIR)/Materialdaten/Gypsum Board.m6

    [IDENTIFICATION]
      NAME                     = Gypsum Board
      COLOUR                   = #ffff8040
      UNIQUE_ID                = 0


  [MATERIAL]
    EXTERNAL                 = $(PROJECT_DIR)/Materialdaten/Spruce_radial (from Saxony) mue= 50 lbd_dry=0,1.m6

    [IDENTIFICATION]
      NAME                     = Spruce_radial (from Saxony) mue= 50 lbd_dry=0,1
      COLOUR                   = #ffaa5555
      UNIQUE_ID                = 0


  [MATERIAL]
    EXTERNAL                 = $(PROJECT_DIR)/Materialdaten/Bitumen.m6

    [IDENTIFICATION]
      NAME                     = Bitumen
      COLOUR                   = #ff5020a0
      UNIQUE_ID                = 0



; ******************************************************************************


[CONDITIONS]

  [WALLS]

    [WALL_DATA]
      NAME                     = Wand - Nord
      ORIENTATION              = 0 Deg
      INCLINATION              = 90 Deg
      LATITUDE                 = 53.53 Deg
      WALLAREA                 = 0 mm2

    [WALL_DATA]
      NAME                     = Wand - Ost
      ORIENTATION              = 90 Deg
      INCLINATION              = 90 Deg
      LATITUDE                 = 53.53 Deg
      WALLAREA                 = 0 mm2

    [WALL_DATA]
      NAME                     = Wand - Sued
      ORIENTATION              = 180 Deg
      INCLINATION              = 90 Deg
      LATITUDE                 = 53.53 Deg
      WALLAREA                 = 0 mm2

    [WALL_DATA]
      NAME                     = Wand - West
      ORIENTATION              = 270 Deg
      INCLINATION              = 90 Deg
      LATITUDE                 = 53.53 Deg
      WALLAREA                 = 0 mm2

    [WALL_DATA]
      NAME                     = Dach - horizontal
      ORIENTATION              = 90 Deg
      INCLINATION              = 0 Deg
      LATITUDE                 = 53.53 Deg
      WALLAREA                 = 0 mm2

    [WALL_DATA]
      NAME                     = Dach - 45 Grad, West
      ORIENTATION              = 270 Deg
      INCLINATION              = 45 Deg
      LATITUDE                 = 53.53 Deg
      WALLAREA                 = 0 mm2



  [CLIMATE_CONDITIONS]

    [CLIMATE_COND]
      TYPE                     = TEMPER
      NAME                     = Inside T
      KIND                     = CONSTANT
      CONSTVALUE               = 20 C

    [CLIMATE_COND]
      TYPE                     = RELHUM
      NAME                     = Inside RH
      KIND                     = CONSTANT
      CONSTVALUE               = 50 %

    [CLIMATE_COND]
      TYPE                     = TEMPER
      NAME                     = 01_Bremerhaven: Temperature
      KIND                     = DATLINEAR
      FILENAME                 = $(PROJECT_DIR)/Klimadaten/Temperature.ccd
      USE_INTERPOLATION        = yes
      EXTEND_DATA              = yes
      CYCLIC_DATA              = yes

    [CLIMATE_COND]
      TYPE                     = RELHUM
      NAME                     = 01_Bremerhaven: Relative humidity
      KIND                     = DATLINEAR
      FILENAME                 = $(PROJECT_DIR)/Klimadaten/RelativeHumidity.ccd
      USE_INTERPOLATION        = yes
      EXTEND_DATA              = yes
      CYCLIC_DATA              = yes

    [CLIMATE_COND]
      TYPE                     = HORRAIN
      NAME                     = 01_Bremerhaven: Rain flux density on a horizontal plane
      KIND                     = DATLINEAR
      FILENAME                 = $(PROJECT_DIR)/Klimadaten/VerticalRain.ccd
      USE_INTERPOLATION        = yes
      EXTEND_DATA              = yes
      CYCLIC_DATA              = yes

    [CLIMATE_COND]
      TYPE                     = WINDDIR
      NAME                     = 01_Bremerhaven: Wind direction, North=0 Deg, East=90 Deg, ...
      KIND                     = DATLINEAR
      FILENAME                 = $(PROJECT_DIR)/Klimadaten/WindDirection.ccd
      USE_INTERPOLATION        = yes
      EXTEND_DATA              = yes
      CYCLIC_DATA              = yes

    [CLIMATE_COND]
      TYPE                     = WINDVEL
      NAME                     = 01_Bremerhaven: Wind velocity
      KIND                     = DATLINEAR
      FILENAME                 = $(PROJECT_DIR)/Klimadaten/WindVelocity.ccd
      USE_INTERPOLATION        = yes
      EXTEND_DATA              = yes
      CYCLIC_DATA              = yes

    [CLIMATE_COND]
      TYPE                     = DIRRAD
      NAME                     = 01_Bremerhaven: Direct sun radiation (short wave component)
      KIND                     = DATLINEAR
      FILENAME                 = $(PROJECT_DIR)/Klimadaten/DirectRadiation.ccd
      USE_INTERPOLATION        = yes
      EXTEND_DATA              = yes
      CYCLIC_DATA              = yes

    [CLIMATE_COND]
      TYPE                     = DIFRAD
      NAME                     = 01_Bremerhaven: Diffuse sun radiation (short wave component)
      KIND                     = DATLINEAR
      FILENAME                 = $(PROJECT_DIR)/Klimadaten/DiffuseRadiation.ccd
      USE_INTERPOLATION        = yes
      EXTEND_DATA              = yes
      CYCLIC_DATA              = yes

    [CLIMATE_COND]
      TYPE                     = SKYEMISS
      NAME                     = 01_Bremerhaven: Atmospheric counter radiation
      KIND                     = DATLINEAR
      FILENAME                 = $(PROJECT_DIR)/Klimadaten/SkyRadiation.ccd
      USE_INTERPOLATION        = yes
      EXTEND_DATA              = yes
      CYCLIC_DATA              = yes



  [BOUNDARY_CONDITIONS]

    [BOUND_COND]
      TYPE                     = HEATCOND
      NAME                     = HeatTransfer innen 8 W/m2K
      KIND                     = EXCHANGE
      EXCOEFF                  = 8 W/m2K
      TEMPER                   = Inside T

    [BOUND_COND]
      TYPE                     = VAPDIFF
      NAME                     = VaporTransfer innen
      KIND                     = EXCHANGE
      EXCOEFF                  = 3e-08 s/m
      SD_VALUE                 = 0 m
      TEMPER                   = Inside T
      RELHUM                   = Inside RH

    [BOUND_COND]
      TYPE                     = HEATCOND
      NAME                     = Bremerhaven: Heat conduction 19 W/m2K
      KIND                     = EXCHANGE
      EXCOEFF                  = 19 W/m2K
      TEMPER                   = 01_Bremerhaven: Temperature

    [BOUND_COND]
      TYPE                     = VAPDIFF
      NAME                     = Bremerhaven: Vapor diffusion
      KIND                     = EXCHANGE
      EXCOEFF                  = 2e-06 s/m
      SD_VALUE                 = 0 m
      TEMPER                   = 01_Bremerhaven: Temperature
      RELHUM                   = 01_Bremerhaven: Relative humidity

    [BOUND_COND]
      TYPE                     = LOWRAD
      NAME                     = Bremerhaven: LW Strahlung WAND-West
      KIND                     = LRADCOMP
      SUREMISS                 = 0.9 -
      WALLDATA                 = Wand - West
      SKYEMISS                 = 01_Bremerhaven: Atmospheric counter radiation

    [BOUND_COND]
      TYPE                     = SHWRAD
      NAME                     = Bremerhaven: KW Strahlung NORD
      KIND                     = SUNRADM
      SURABSOR                 = 0.6 -
      GRDREFLE                 = 0.2 -
      WALLDATA                 = Wand - Nord
      DIRRAD                   = 01_Bremerhaven: Direct sun radiation (short wave component)
      DIFRAD                   = 01_Bremerhaven: Diffuse sun radiation (short wave component)

    [BOUND_COND]
      TYPE                     = RAIN
      NAME                     = Bremerhaven: Regen NORD
      KIND                     = STDRAIN
      EXPCOEFF                 = 1 -
      MINRTEMP                 = -2 C
      MINRFLUX                 = 0 l/m2s
      WALLDATA                 = Wand - Nord
      TEMPER                   = 01_Bremerhaven: Temperature
      RELHUM                   = 01_Bremerhaven: Relative humidity
      HORRAIN                  = 01_Bremerhaven: Rain flux density on a horizontal plane
      WINDDIR                  = 01_Bremerhaven: Wind direction, North=0 Deg, East=90 Deg, ...
      WINDVEL                  = 01_Bremerhaven: Wind velocity

    [BOUND_COND]
      TYPE                     = SHWRAD
      NAME                     = Bremerhaven: KW Strahlung OST
      KIND                     = SUNRADM
      SURABSOR                 = 0.6 -
      GRDREFLE                 = 0.2 -
      WALLDATA                 = Wand - Ost
      DIRRAD                   = 01_Bremerhaven: Direct sun radiation (short wave component)
      DIFRAD                   = 01_Bremerhaven: Diffuse sun radiation (short wave component)

    [BOUND_COND]
      TYPE                     = RAIN
      NAME                     = Bremerhaven: Regen OST
      KIND                     = STDRAIN
      EXPCOEFF                 = 1 -
      MINRTEMP                 = -2 C
      MINRFLUX                 = 0 l/m2s
      WALLDATA                 = Wand - Ost
      TEMPER                   = 01_Bremerhaven: Temperature
      RELHUM                   = 01_Bremerhaven: Relative humidity
      HORRAIN                  = 01_Bremerhaven: Rain flux density on a horizontal plane
      WINDDIR                  = 01_Bremerhaven: Wind direction, North=0 Deg, East=90 Deg, ...
      WINDVEL                  = 01_Bremerhaven: Wind velocity

    [BOUND_COND]
      TYPE                     = SHWRAD
      NAME                     = Bremerhaven: KW Strahlung SUED
      KIND                     = SUNRADM
      SURABSOR                 = 0.6 -
      GRDREFLE                 = 0.2 -
      WALLDATA                 = Wand - Sued
      DIRRAD                   = 01_Bremerhaven: Direct sun radiation (short wave component)
      DIFRAD                   = 01_Bremerhaven: Diffuse sun radiation (short wave component)

    [BOUND_COND]
      TYPE                     = RAIN
      NAME                     = Bremerhaven: Regen SUED
      KIND                     = STDRAIN
      EXPCOEFF                 = 1 -
      MINRTEMP                 = -2 C
      MINRFLUX                 = 0 l/m2s
      WALLDATA                 = Wand - Sued
      TEMPER                   = 01_Bremerhaven: Temperature
      RELHUM                   = 01_Bremerhaven: Relative humidity
      HORRAIN                  = 01_Bremerhaven: Rain flux density on a horizontal plane
      WINDDIR                  = 01_Bremerhaven: Wind direction, North=0 Deg, East=90 Deg, ...
      WINDVEL                  = 01_Bremerhaven: Wind velocity

    [BOUND_COND]
      TYPE                     = SHWRAD
      NAME                     = Bremerhaven: KW Strahlung WEST
      KIND                     = SUNRADM
      SURABSOR                 = 0.6 -
      GRDREFLE                 = 0.2 -
      WALLDATA                 = Wand - West
      DIRRAD                   = 01_Bremerhaven: Direct sun radiation (short wave component)
      DIFRAD                   = 01_Bremerhaven: Diffuse sun radiation (short wave component)

    [BOUND_COND]
      TYPE                     = RAIN
      NAME                     = Bremerhaven: Regen WEST
      KIND                     = STDRAIN
      EXPCOEFF                 = 1 -
      MINRTEMP                 = -2 C
      MINRFLUX                 = 0 l/m2s
      WALLDATA                 = Wand - West
      TEMPER                   = 01_Bremerhaven: Temperature
      RELHUM                   = 01_Bremerhaven: Relative humidity
      HORRAIN                  = 01_Bremerhaven: Rain flux density on a horizontal plane
      WINDDIR                  = 01_Bremerhaven: Wind direction, North=0 Deg, East=90 Deg, ...
      WINDVEL                  = 01_Bremerhaven: Wind velocity

    [BOUND_COND]
      TYPE                     = SHWRAD
      NAME                     = Bremerhaven: KW Strahlung DACH-hor
      KIND                     = SUNRADM
      SURABSOR                 = 0.6 -
      GRDREFLE                 = 0.2 -
      WALLDATA                 = Dach - horizontal
      DIRRAD                   = 01_Bremerhaven: Direct sun radiation (short wave component)
      DIFRAD                   = 01_Bremerhaven: Diffuse sun radiation (short wave component)

    [BOUND_COND]
      TYPE                     = RAIN
      NAME                     = Bremerhaven: Regen DACH-hor
      KIND                     = STDRAIN
      EXPCOEFF                 = 1 -
      MINRTEMP                 = -2 C
      MINRFLUX                 = 0 l/m2s
      WALLDATA                 = Dach - horizontal
      TEMPER                   = 01_Bremerhaven: Temperature
      RELHUM                   = 01_Bremerhaven: Relative humidity
      HORRAIN                  = 01_Bremerhaven: Rain flux density on a horizontal plane
      WINDDIR                  = 01_Bremerhaven: Wind direction, North=0 Deg, East=90 Deg, ...
      WINDVEL                  = 01_Bremerhaven: Wind velocity

    [BOUND_COND]
      TYPE                     = LOWRAD
      NAME                     = Bremerhaven: LW Strahlung DACH-hor
      KIND                     = LRADCOMP
      SUREMISS                 = 0.9 -
      WALLDATA                 = Dach - horizontal
      SKYEMISS                 = 01_Bremerhaven: Atmospheric counter radiation

    [BOUND_COND]
      TYPE                     = HEATCOND
      NAME                     = HeatTransfer innen DACH 10 W/m2K
      KIND                     = EXCHANGE
      EXCOEFF                  = 10 W/m2K
      TEMPER                   = Inside T



  [CONTACT_CONDITIONS]

    [CONTACT_COND]
      TYPE                     = FOIL_ADAPTIVE
      NAME                     = SIGA Majrex
      KIND                     = DIRECTION_DEPENDENT
      WEIGHT_FACTOR_POS        = 0.52 -
      WEIGHT_FACTOR_NEG        = 0.55 -
      SCALING_A_POS            = 0.11795 -
      SCALING_B_POS            = 0.010393 -
      SCALING_C_POS            = -0.00038823 -
      SCALING_A_NEG            = -0.6271 -
      SCALING_B_NEG            = 0.042838 -
      SCALING_C_NEG            = -0.0007187 -
      FUNCTION                 = sd+(rh)
          0                0.15             0.4              0.5              0.7              0.75             0.8              0.85             0.9              0.99             1                
          35               35               12.97            12.97            3.52             3.52             2.36             1.16             1.16             1.16             1.16             
      FUNCTION                 = sd-(rh)
          0                0.15             0.4              0.5              0.7              0.75             0.8              0.85             0.9              0.99             1                
          35               35               9.45             9.45             1.6              1.6              1.39             1.16             1.16             1.16             1.16             
      SD_POSITIVE_DIRECTION    = yes
      FOIL_NAME                = SIGA Majrex

    [CONTACT_COND]
      TYPE                     = FOIL
      NAME                     = Unterdachbahn Tyvek
      VAPDIFFRES               = 0.088 m
      FOIL_NAME                = DuPont Tyvek DPT




  [DEFAULT_CONDITIONS]

    DEFAULT_TEMPERATURE      = 20 C
    DEFAULT_RELHUM           = 80 %

; ******************************************************************************


[DISCRETISATION]

  GEOMETRY                 = PLANE2D
  X_STEPS                  = 0.001 0.00149975 0.00224926 0.00337333 0.00505917 0.0075875 0.0113794 0.0170663 0.0255952 0.0301268 0.0301268 0.0301268 0.0255952 0.0170663 0.0113794 0.0075875 0.00505917 0.00337333 0.00224926 0.00149975 0.001 0.001 0.00149975 0.00166683 0.00166683 0.00166683 0.00149975 0.001 0.001 0.0015 0.0015 0.0015 0.0015 0.001 0.001 0.00149975 0.00224926 0.00337333 0.00505917 0.00840924 0.00840924 0.00840924 0.00840924 0.00505917 0.00337333 0.00224926 0.00149975 0.001 0.001 0.001 0.001 0.001 0.05 0.05 0.001 0.00149975 0.00224926 0.00337333 0.00505917 0.0075875 0.0113794 0.0170663 0.0255952 0.0301268 0.0301268 0.0301268 0.0255952 0.0170663 0.0113794 0.0075875 0.00505917 0.00337333 0.00224926 0.00149975 0.001 0.001 0.00149975 0.00166683 0.00166683 0.00166683 0.00149975 0.001 0.001 0.0015 0.0015 0.0015 0.0015 0.001 0.001 0.00149975 0.00224926 0.00337333 0.00505917 0.00840924 0.00840924 0.00840924 0.00840924 0.00505917 0.00337333 0.00224926 0.00149975 0.001 0.001 0.001 0.001 0.001 0.05 0.05 0.001 0.00149975 0.00224926 0.00337333 0.00505917 0.0075875 0.0113794 0.0170663 0.0255952 0.0301268 0.0301268 0.0301268 0.0255952 0.0170663 0.0113794 0.0075875 0.00505917 0.00337333 0.00224926 0.00149975 0.001 0.001 0.00149975 0.00166683 0.00166683 0.00166683 0.00149975 0.001 0.001 0.0015 0.0015 0.0015 0.0015 0.001 0.001 0.00149975 0.00224926 0.00337333 0.00505917 0.00840924 0.00840924 0.00840924 0.00840924 0.00505917 0.00337333 0.00224926 0.00149975 0.001 0.001 0.001 0.001 0.001 0.05 0.05 0.001 0.00149975 0.00224926 0.00337333 0.00505917 0.0075875 0.0113794 0.0170663 0.0255952 0.0301268 0.0301268 0.0301268 0.0255952 0.0170663 0.0113794 0.0075875 0.00505917 0.00337333 0.00224926 0.00149975 0.001 0.001 0.00149975 0.00166683 0.00166683 0.00166683 0.00149975 0.001 0.001 0.0015 0.0015 0.0015 0.0015 0.001 0.001 0.00149975 0.00224926 0.00337333 0.00505917 0.00840924 0.00840924 0.00840924 0.00840924 0.00505917 0.00337333 0.00224926 0.00149975 0.001 0.001 0.001 0.001 0.001 0.05 0.05 0.001 0.001 0.001 0.001 0.001 0.00149975 0.00224926 0.00387549 0.00387549 0.00387549 0.00387549 0.00224926 0.00149975 0.001 0.001 0.00149975 0.00224926 0.00337333 0.00505917 0.0075875 0.0113794 0.0189258 0.0189258 0.0189258 0.0189258 0.0113794 0.0075875 0.00505917 0.00337333 0.00224926 0.00149975 0.001 0.001 0.00149975 0.00224926 0.00387549 0.00387549 0.00387549 0.00387549 0.00224926 0.00149975 0.001 m
  Y_STEPS                  = 1 m
  Z_STEPS                  = 1 m
  THETA_Z                  = 0
  PIE_SLICE_ANGLE          = 360

; ******************************************************************************


[OUTPUTS]

  [GENERAL]
    OUTPUT_FOLDER            = $(PROJECT_DIR)/RealKlima.results
    MAX_HYG_RELHUM           = 95 %
    EXP_REF_TEMPER           = 0 C
    EXP_REF_RELHUM           = 60 %
    THAW_BEGIN               = 0
    FREEZE_BEGIN             = 0.01 ---


  [GRIDS]

    [OUTPUT_GRID]
      NAME                     = 30min
      INTERVAL                 = 0 d            30 min         


  [FORMATS]

    [OUTPUT_FORMAT]
      NAME                     = Feuchtigkeit Gesamt (int)
      TYPE                     = FIELD
      FIELD_TYPE               = MOISTURE
      SPACE_TYPE               = INTEGRAL
      TIME_TYPE                = NONE
      TIME_UNIT                = d
      VALUE_UNIT               = kg
      PRECISION                = 9
      WIDTH                    = 12
      FORMAT                   = DEFAULT
      BINARY                   = no

    [OUTPUT_FORMAT]
      NAME                     = Feuchtestrom
      TYPE                     = FLUX
      FLUX_TYPE                = MOISTFLUX
      SPACE_TYPE               = SINGLE
      TIME_TYPE                = NONE
      TIME_UNIT                = d
      VALUE_UNIT               = g/m2h
      PRECISION                = 9
      WIDTH                    = 12
      FORMAT                   = DEFAULT
      BINARY                   = no

    [OUTPUT_FORMAT]
      NAME                     = Schlagregen
      TYPE                     = FLUX
      FLUX_TYPE                = NORMRAIN
      SPACE_TYPE               = SINGLE
      TIME_TYPE                = NONE
      TIME_UNIT                = d
      VALUE_UNIT               = g/m2h
      PRECISION                = 9
      WIDTH                    = 12
      FORMAT                   = DEFAULT
      BINARY                   = yes

    [OUTPUT_FORMAT]
      NAME                     = Schlagregen (time-int)
      TYPE                     = FLUX
      FLUX_TYPE                = NORMRAIN
      SPACE_TYPE               = SINGLE
      TIME_TYPE                = INTEGRAL
      TIME_UNIT                = d
      VALUE_UNIT               = kg/m2
      PRECISION                = 9
      WIDTH                    = 12
      FORMAT                   = DEFAULT
      BINARY                   = no

    [OUTPUT_FORMAT]
      NAME                     = Saettigungsgrad
      TYPE                     = FIELD
      FIELD_TYPE               = SATDEGREE
      SPACE_TYPE               = SINGLE
      TIME_TYPE                = NONE
      TIME_UNIT                = d
      VALUE_UNIT               = %
      PRECISION                = 9
      WIDTH                    = 12
      FORMAT                   = DEFAULT
      BINARY                   = no

    [OUTPUT_FORMAT]
      NAME                     = SW-Radiation time-integrated
      TYPE                     = FLUX
      FLUX_TYPE                = SHWRAD
      SPACE_TYPE               = MEAN
      TIME_TYPE                = INTEGRAL
      TIME_UNIT                = d
      VALUE_UNIT               = kWh/m2
      PRECISION                = 9
      WIDTH                    = 12
      FORMAT                   = DEFAULT
      BINARY                   = no

    [OUTPUT_FORMAT]
      NAME                     = LW-Radiation time-integrated
      TYPE                     = FLUX
      FLUX_TYPE                = LWRAD
      SPACE_TYPE               = MEAN
      TIME_TYPE                = INTEGRAL
      TIME_UNIT                = d
      VALUE_UNIT               = kWh/m2
      PRECISION                = 9
      WIDTH                    = 12
      FORMAT                   = DEFAULT
      BINARY                   = no


  [FILES]

    [OUTPUT_FILE]
      NAME                     = flux_moisture_ROOF.out
      OUTPUT_GRID              = 30min
      OUTPUT_FORMAT            = Feuchtestrom

    [OUTPUT_FILE]
      NAME                     = flux_rain_normal_ROOF.out
      OUTPUT_GRID              = 30min
      OUTPUT_FORMAT            = Schlagregen

    [OUTPUT_FILE]
      NAME                     = flux_rain_normal_integral_ROOF.out
      OUTPUT_GRID              = 30min
      OUTPUT_FORMAT            = Schlagregen (time-int)

    [OUTPUT_FILE]
      NAME                     = flux_SW-rad_ROOF.out
      OUTPUT_GRID              = 30min
      OUTPUT_FORMAT            = SW-Radiation time-integrated

    [OUTPUT_FILE]
      NAME                     = flux_LW-rad_ROOF.out
      OUTPUT_GRID              = 30min
      OUTPUT_FORMAT            = LW-Radiation time-integrated

    [OUTPUT_FILE]
      NAME                     = moist_mass_integral_ROOF.out
      OUTPUT_GRID              = 30min
      OUTPUT_FORMAT            = Feuchtigkeit Gesamt (int)

    [OUTPUT_FILE]
      NAME                     = flux_moisture_NORTH.out
      OUTPUT_GRID              = 30min
      OUTPUT_FORMAT            = Feuchtestrom

    [OUTPUT_FILE]
      NAME                     = flux_rain_normal_NORTH.out
      OUTPUT_GRID              = 30min
      OUTPUT_FORMAT            = Schlagregen

    [OUTPUT_FILE]
      NAME                     = flux_rain_normal_integral_NORTH.out
      OUTPUT_GRID              = 30min
      OUTPUT_FORMAT            = Schlagregen (time-int)

    [OUTPUT_FILE]
      NAME                     = flux_SW-rad_NORTH.out
      OUTPUT_GRID              = 30min
      OUTPUT_FORMAT            = SW-Radiation time-integrated

    [OUTPUT_FILE]
      NAME                     = flux_LW-rad_NORTH.out
      OUTPUT_GRID              = 30min
      OUTPUT_FORMAT            = LW-Radiation time-integrated

    [OUTPUT_FILE]
      NAME                     = moist_mass_integral_NORTH.out
      OUTPUT_GRID              = 30min
      OUTPUT_FORMAT            = Feuchtigkeit Gesamt (int)

    [OUTPUT_FILE]
      NAME                     = flux_moisture_EAST.out
      OUTPUT_GRID              = 30min
      OUTPUT_FORMAT            = Feuchtestrom

    [OUTPUT_FILE]
      NAME                     = flux_rain_normal_EAST.out
      OUTPUT_GRID              = 30min
      OUTPUT_FORMAT            = Schlagregen

    [OUTPUT_FILE]
      NAME                     = flux_rain_normal_integral_EAST.out
      OUTPUT_GRID              = 30min
      OUTPUT_FORMAT            = Schlagregen (time-int)

    [OUTPUT_FILE]
      NAME                     = flux_SW-rad_EAST.out
      OUTPUT_GRID              = 30min
      OUTPUT_FORMAT            = SW-Radiation time-integrated

    [OUTPUT_FILE]
      NAME                     = flux_LW-rad_EAST.out
      OUTPUT_GRID              = 30min
      OUTPUT_FORMAT            = LW-Radiation time-integrated

    [OUTPUT_FILE]
      NAME                     = moist_mass_integral_EAST.out
      OUTPUT_GRID              = 30min
      OUTPUT_FORMAT            = Feuchtigkeit Gesamt (int)

    [OUTPUT_FILE]
      NAME                     = flux_moisture_SOUTH.out
      OUTPUT_GRID              = 30min
      OUTPUT_FORMAT            = Feuchtestrom

    [OUTPUT_FILE]
      NAME                     = flux_rain_normal_SOUTH.out
      OUTPUT_GRID              = 30min
      OUTPUT_FORMAT            = Schlagregen

    [OUTPUT_FILE]
      NAME                     = flux_rain_normal_integral_SOUTH.out
      OUTPUT_GRID              = 30min
      OUTPUT_FORMAT            = Schlagregen (time-int)

    [OUTPUT_FILE]
      NAME                     = flux_SW-rad_SOUTH.out
      OUTPUT_GRID              = 30min
      OUTPUT_FORMAT            = SW-Radiation time-integrated

    [OUTPUT_FILE]
      NAME                     = flux_LW-rad_SOUTH.out
      OUTPUT_GRID              = 30min
      OUTPUT_FORMAT            = LW-Radiation time-integrated

    [OUTPUT_FILE]
      NAME                     = moist_mass_integral_SOUTH.out
      OUTPUT_GRID              = 30min
      OUTPUT_FORMAT            = Feuchtigkeit Gesamt (int)

    [OUTPUT_FILE]
      NAME                     = flux_moisture_WEST.out
      OUTPUT_GRID              = 30min
      OUTPUT_FORMAT            = Feuchtestrom

    [OUTPUT_FILE]
      NAME                     = flux_rain_normal_WEST.out
      OUTPUT_GRID              = 30min
      OUTPUT_FORMAT            = Schlagregen

    [OUTPUT_FILE]
      NAME                     = flux_rain_normal_integral_WEST.out
      OUTPUT_GRID              = 30min
      OUTPUT_FORMAT            = Schlagregen (time-int)

    [OUTPUT_FILE]
      NAME                     = flux_SW-rad_WEST.out
      OUTPUT_GRID              = 30min
      OUTPUT_FORMAT            = SW-Radiation time-integrated

    [OUTPUT_FILE]
      NAME                     = flux_LW-rad_WEST.out
      OUTPUT_GRID              = 30min
      OUTPUT_FORMAT            = LW-Radiation time-integrated

    [OUTPUT_FILE]
      NAME                     = moist_mass_integral_WEST.out
      OUTPUT_GRID              = 30min
      OUTPUT_FORMAT            = Feuchtigkeit Gesamt (int)



; ******************************************************************************


[ASSIGNMENTS]

  [SELECTION]
    TYPE                     = MATERIAL
    RANGE                    = 0 0 20 0
    NAME                     = Altbauziegel Dresden ZE
    LOCATION                 = ELEMENT 

  [SELECTION]
    TYPE                     = MATERIAL
    RANGE                    = 21 0 27 0
    NAME                     = Levelling Plaster
    LOCATION                 = ELEMENT 

  [SELECTION]
    TYPE                     = MATERIAL
    RANGE                    = 54 0 74 0
    NAME                     = Altbauziegel Dresden ZE
    LOCATION                 = ELEMENT 

  [SELECTION]
    TYPE                     = MATERIAL
    RANGE                    = 75 0 81 0
    NAME                     = Levelling Plaster
    LOCATION                 = ELEMENT 

  [SELECTION]
    TYPE                     = MATERIAL
    RANGE                    = 108 0 128 0
    NAME                     = Altbauziegel Dresden ZE
    LOCATION                 = ELEMENT 

  [SELECTION]
    TYPE                     = MATERIAL
    RANGE                    = 129 0 135 0
    NAME                     = Levelling Plaster
    LOCATION                 = ELEMENT 

  [SELECTION]
    TYPE                     = MATERIAL
    RANGE                    = 162 0 182 0
    NAME                     = Altbauziegel Dresden ZE
    LOCATION                 = ELEMENT 

  [SELECTION]
    TYPE                     = MATERIAL
    RANGE                    = 183 0 189 0
    NAME                     = Levelling Plaster
    LOCATION                 = ELEMENT 

  [SELECTION]
    TYPE                     = MATERIAL
    RANGE                    = 216 0 219 0
    NAME                     = Altbauziegel Dresden ZE
    LOCATION                 = ELEMENT 

  [SELECTION]
    TYPE                     = MATERIAL
    RANGE                    = 220 0 229 0
    NAME                     = Levelling Plaster
    LOCATION                 = ELEMENT 

  [SELECTION]
    TYPE                     = MATERIAL
    RANGE                    = 28 0 33 0
    NAME                     = Calsitherm KP Glue Mortar
    LOCATION                 = ELEMENT 

  [SELECTION]
    TYPE                     = MATERIAL
    RANGE                    = 82 0 87 0
    NAME                     = Calsitherm KP Glue Mortar
    LOCATION                 = ELEMENT 

  [SELECTION]
    TYPE                     = MATERIAL
    RANGE                    = 136 0 141 0
    NAME                     = Calsitherm KP Glue Mortar
    LOCATION                 = ELEMENT 

  [SELECTION]
    TYPE                     = MATERIAL
    RANGE                    = 190 0 195 0
    NAME                     = Calsitherm KP Glue Mortar
    LOCATION                 = ELEMENT 

  [SELECTION]
    TYPE                     = MATERIAL
    RANGE                    = 230 0 247 0
    NAME                     = Calsitherm KP Glue Mortar
    LOCATION                 = ELEMENT 

  [SELECTION]
    TYPE                     = MATERIAL
    RANGE                    = 34 0 47 0
    NAME                     = Calsitherm Climate Board WF
    LOCATION                 = ELEMENT 

  [SELECTION]
    TYPE                     = MATERIAL
    RANGE                    = 88 0 101 0
    NAME                     = Calsitherm Climate Board WF
    LOCATION                 = ELEMENT 

  [SELECTION]
    TYPE                     = MATERIAL
    RANGE                    = 142 0 155 0
    NAME                     = Calsitherm Climate Board WF
    LOCATION                 = ELEMENT 

  [SELECTION]
    TYPE                     = MATERIAL
    RANGE                    = 196 0 209 0
    NAME                     = Calsitherm Climate Board WF
    LOCATION                 = ELEMENT 

  [SELECTION]
    TYPE                     = MATERIAL
    RANGE                    = 248 0 257 0
    NAME                     = Calsitherm Climate Board WF
    LOCATION                 = ELEMENT 

  [SELECTION]
    TYPE                     = MATERIAL
    RANGE                    = 48 0 51 0
    NAME                     = Calsitherm KP Lime Plaster
    LOCATION                 = ELEMENT 

  [SELECTION]
    TYPE                     = MATERIAL
    RANGE                    = 102 0 105 0
    NAME                     = Calsitherm KP Lime Plaster
    LOCATION                 = ELEMENT 

  [SELECTION]
    TYPE                     = MATERIAL
    RANGE                    = 156 0 159 0
    NAME                     = Calsitherm KP Lime Plaster
    LOCATION                 = ELEMENT 

  [SELECTION]
    TYPE                     = MATERIAL
    RANGE                    = 210 0 213 0
    NAME                     = Calsitherm KP Lime Plaster
    LOCATION                 = ELEMENT 

  [SELECTION]
    TYPE                     = MATERIAL
    RANGE                    = 216 0 219 0
    NAME                     = Bitumen
    LOCATION                 = ELEMENT 

  [SELECTION]
    TYPE                     = MATERIAL
    RANGE                    = 220 0 229 0
    NAME                     = Spruce_radial (from Saxony) mue= 50 lbd_dry=0,1
    LOCATION                 = ELEMENT 

  [SELECTION]
    TYPE                     = MATERIAL
    RANGE                    = 230 0 247 0
    NAME                     = Mineral Wool 035
    LOCATION                 = ELEMENT 

  [SELECTION]
    TYPE                     = MATERIAL
    RANGE                    = 248 0 257 0
    NAME                     = Gypsum Board
    LOCATION                 = ELEMENT 

  [SELECTION]
    TYPE                     = BOUNDARYCOND
    RANGE                    = 257 0 257 0
    NAME                     = HeatTransfer innen DACH 10 W/m2K
    LOCATION                 = RIGHT 
    CONDITION_TYPE           = HEATCOND

  [SELECTION]
    TYPE                     = BOUNDARYCOND
    RANGE                    = 257 0 257 0
    NAME                     = VaporTransfer innen
    LOCATION                 = RIGHT 
    CONDITION_TYPE           = VAPDIFF

  [SELECTION]
    TYPE                     = BOUNDARYCOND
    RANGE                    = 0 0 0 0
    NAME                     = Bremerhaven: Heat conduction 19 W/m2K
    LOCATION                 = LEFT 
    CONDITION_TYPE           = HEATCOND

  [SELECTION]
    TYPE                     = BOUNDARYCOND
    RANGE                    = 0 0 0 0
    NAME                     = Bremerhaven: Vapor diffusion
    LOCATION                 = LEFT 
    CONDITION_TYPE           = VAPDIFF

  [SELECTION]
    TYPE                     = BOUNDARYCOND
    RANGE                    = 0 0 0 0
    NAME                     = Bremerhaven: LW Strahlung WAND-West
    LOCATION                 = LEFT 
    CONDITION_TYPE           = LOWRAD

  [SELECTION]
    TYPE                     = BOUNDARYCOND
    RANGE                    = 54 0 54 0
    NAME                     = Bremerhaven: Heat conduction 19 W/m2K
    LOCATION                 = LEFT 
    CONDITION_TYPE           = HEATCOND

  [SELECTION]
    TYPE                     = BOUNDARYCOND
    RANGE                    = 54 0 54 0
    NAME                     = Bremerhaven: Vapor diffusion
    LOCATION                 = LEFT 
    CONDITION_TYPE           = VAPDIFF

  [SELECTION]
    TYPE                     = BOUNDARYCOND
    RANGE                    = 54 0 54 0
    NAME                     = Bremerhaven: LW Strahlung WAND-West
    LOCATION                 = LEFT 
    CONDITION_TYPE           = LOWRAD

  [SELECTION]
    TYPE                     = BOUNDARYCOND
    RANGE                    = 108 0 108 0
    NAME                     = Bremerhaven: Heat conduction 19 W/m2K
    LOCATION                 = LEFT 
    CONDITION_TYPE           = HEATCOND

  [SELECTION]
    TYPE                     = BOUNDARYCOND
    RANGE                    = 108 0 108 0
    NAME                     = Bremerhaven: Vapor diffusion
    LOCATION                 = LEFT 
    CONDITION_TYPE           = VAPDIFF

  [SELECTION]
    TYPE                     = BOUNDARYCOND
    RANGE                    = 108 0 108 0
    NAME                     = Bremerhaven: LW Strahlung WAND-West
    LOCATION                 = LEFT 
    CONDITION_TYPE           = LOWRAD

  [SELECTION]
    TYPE                     = BOUNDARYCOND
    RANGE                    = 162 0 162 0
    NAME                     = Bremerhaven: Heat conduction 19 W/m2K
    LOCATION                 = LEFT 
    CONDITION_TYPE           = HEATCOND

  [SELECTION]
    TYPE                     = BOUNDARYCOND
    RANGE                    = 162 0 162 0
    NAME                     = Bremerhaven: Vapor diffusion
    LOCATION                 = LEFT 
    CONDITION_TYPE           = VAPDIFF

  [SELECTION]
    TYPE                     = BOUNDARYCOND
    RANGE                    = 162 0 162 0
    NAME                     = Bremerhaven: LW Strahlung WAND-West
    LOCATION                 = LEFT 
    CONDITION_TYPE           = LOWRAD

  [SELECTION]
    TYPE                     = BOUNDARYCOND
    RANGE                    = 0 0 0 0
    NAME                     = Bremerhaven: KW Strahlung NORD
    LOCATION                 = LEFT 
    CONDITION_TYPE           = SHWRAD

  [SELECTION]
    TYPE                     = BOUNDARYCOND
    RANGE                    = 0 0 0 0
    NAME                     = Bremerhaven: Regen NORD
    LOCATION                 = LEFT 
    CONDITION_TYPE           = RAIN

  [SELECTION]
    TYPE                     = BOUNDARYCOND
    RANGE                    = 54 0 54 0
    NAME                     = Bremerhaven: KW Strahlung OST
    LOCATION                 = LEFT 
    CONDITION_TYPE           = SHWRAD

  [SELECTION]
    TYPE                     = BOUNDARYCOND
    RANGE                    = 54 0 54 0
    NAME                     = Bremerhaven: Regen OST
    LOCATION                 = LEFT 
    CONDITION_TYPE           = RAIN

  [SELECTION]
    TYPE                     = BOUNDARYCOND
    RANGE                    = 108 0 108 0
    NAME                     = Bremerhaven: KW Strahlung SUED
    LOCATION                 = LEFT 
    CONDITION_TYPE           = SHWRAD

  [SELECTION]
    TYPE                     = BOUNDARYCOND
    RANGE                    = 108 0 108 0
    NAME                     = Bremerhaven: Regen SUED
    LOCATION                 = LEFT 
    CONDITION_TYPE           = RAIN

  [SELECTION]
    TYPE                     = BOUNDARYCOND
    RANGE                    = 162 0 162 0
    NAME                     = Bremerhaven: KW Strahlung WEST
    LOCATION                 = LEFT 
    CONDITION_TYPE           = SHWRAD

  [SELECTION]
    TYPE                     = BOUNDARYCOND
    RANGE                    = 162 0 162 0
    NAME                     = Bremerhaven: Regen WEST
    LOCATION                 = LEFT 
    CONDITION_TYPE           = RAIN

  [SELECTION]
    TYPE                     = BOUNDARYCOND
    RANGE                    = 216 0 216 0
    NAME                     = Bremerhaven: KW Strahlung DACH-hor
    LOCATION                 = LEFT 
    CONDITION_TYPE           = SHWRAD

  [SELECTION]
    TYPE                     = BOUNDARYCOND
    RANGE                    = 216 0 216 0
    NAME                     = Bremerhaven: Regen DACH-hor
    LOCATION                 = LEFT 
    CONDITION_TYPE           = RAIN

  [SELECTION]
    TYPE                     = BOUNDARYCOND
    RANGE                    = 216 0 216 0
    NAME                     = Bremerhaven: LW Strahlung DACH-hor
    LOCATION                 = LEFT 
    CONDITION_TYPE           = LOWRAD

  [SELECTION]
    TYPE                     = BOUNDARYCOND
    RANGE                    = 51 0 51 0
    NAME                     = HeatTransfer innen 8 W/m2K
    LOCATION                 = RIGHT 
    CONDITION_TYPE           = HEATCOND

  [SELECTION]
    TYPE                     = BOUNDARYCOND
    RANGE                    = 51 0 51 0
    NAME                     = VaporTransfer innen
    LOCATION                 = RIGHT 
    CONDITION_TYPE           = VAPDIFF

  [SELECTION]
    TYPE                     = BOUNDARYCOND
    RANGE                    = 105 0 105 0
    NAME                     = HeatTransfer innen 8 W/m2K
    LOCATION                 = RIGHT 
    CONDITION_TYPE           = HEATCOND

  [SELECTION]
    TYPE                     = BOUNDARYCOND
    RANGE                    = 105 0 105 0
    NAME                     = VaporTransfer innen
    LOCATION                 = RIGHT 
    CONDITION_TYPE           = VAPDIFF

  [SELECTION]
    TYPE                     = BOUNDARYCOND
    RANGE                    = 159 0 159 0
    NAME                     = HeatTransfer innen 8 W/m2K
    LOCATION                 = RIGHT 
    CONDITION_TYPE           = HEATCOND

  [SELECTION]
    TYPE                     = BOUNDARYCOND
    RANGE                    = 159 0 159 0
    NAME                     = VaporTransfer innen
    LOCATION                 = RIGHT 
    CONDITION_TYPE           = VAPDIFF

  [SELECTION]
    TYPE                     = BOUNDARYCOND
    RANGE                    = 213 0 213 0
    NAME                     = HeatTransfer innen 8 W/m2K
    LOCATION                 = RIGHT 
    CONDITION_TYPE           = HEATCOND

  [SELECTION]
    TYPE                     = BOUNDARYCOND
    RANGE                    = 213 0 213 0
    NAME                     = VaporTransfer innen
    LOCATION                 = RIGHT 
    CONDITION_TYPE           = VAPDIFF

  [SELECTION]
    TYPE                     = BOUNDARYCOND
    RANGE                    = 216 0 216 0
    NAME                     = Bremerhaven: Heat conduction 19 W/m2K
    LOCATION                 = LEFT 
    CONDITION_TYPE           = HEATCOND

  [SELECTION]
    TYPE                     = CONTACTCOND
    RANGE                    = 248 0 248 0
    NAME                     = SIGA Majrex
    LOCATION                 = LEFT 

  [SELECTION]
    TYPE                     = CONTACTCOND
    RANGE                    = 230 0 230 0
    NAME                     = Unterdachbahn Tyvek
    LOCATION                 = LEFT 

  [SELECTION]
    TYPE                     = FIELDOUTPUT
    RANGE                    = 216 0 257 0
    NAME                     = moist_mass_integral_ROOF.out
    LOCATION                 = ELEMENT 

  [SELECTION]
    TYPE                     = FIELDOUTPUT
    RANGE                    = 0 0 51 0
    NAME                     = moist_mass_integral_NORTH.out
    LOCATION                 = ELEMENT 

  [SELECTION]
    TYPE                     = FIELDOUTPUT
    RANGE                    = 54 0 105 0
    NAME                     = moist_mass_integral_EAST.out
    LOCATION                 = ELEMENT 

  [SELECTION]
    TYPE                     = FIELDOUTPUT
    RANGE                    = 108 0 159 0
    NAME                     = moist_mass_integral_SOUTH.out
    LOCATION                 = ELEMENT 

  [SELECTION]
    TYPE                     = FIELDOUTPUT
    RANGE                    = 162 0 213 0
    NAME                     = moist_mass_integral_WEST.out
    LOCATION                 = ELEMENT 

  [SELECTION]
    TYPE                     = FLUXOUTPUT
    RANGE                    = 216 0 216 0
    NAME                     = flux_moisture_ROOF.out
    LOCATION                 = LEFT 

  [SELECTION]
    TYPE                     = FLUXOUTPUT
    RANGE                    = 216 0 216 0
    NAME                     = flux_rain_normal_ROOF.out
    LOCATION                 = LEFT 

  [SELECTION]
    TYPE                     = FLUXOUTPUT
    RANGE                    = 216 0 216 0
    NAME                     = flux_rain_normal_integral_ROOF.out
    LOCATION                 = LEFT 

  [SELECTION]
    TYPE                     = FLUXOUTPUT
    RANGE                    = 216 0 216 0
    NAME                     = flux_SW-rad_ROOF.out
    LOCATION                 = LEFT 

  [SELECTION]
    TYPE                     = FLUXOUTPUT
    RANGE                    = 216 0 216 0
    NAME                     = flux_LW-rad_ROOF.out
    LOCATION                 = LEFT 

  [SELECTION]
    TYPE                     = FLUXOUTPUT
    RANGE                    = 0 0 0 0
    NAME                     = flux_moisture_NORTH.out
    LOCATION                 = LEFT 

  [SELECTION]
    TYPE                     = FLUXOUTPUT
    RANGE                    = 0 0 0 0
    NAME                     = flux_rain_normal_NORTH.out
    LOCATION                 = LEFT 

  [SELECTION]
    TYPE                     = FLUXOUTPUT
    RANGE                    = 0 0 0 0
    NAME                     = flux_rain_normal_integral_NORTH.out
    LOCATION                 = LEFT 

  [SELECTION]
    TYPE                     = FLUXOUTPUT
    RANGE                    = 0 0 0 0
    NAME                     = flux_SW-rad_NORTH.out
    LOCATION                 = LEFT 

  [SELECTION]
    TYPE                     = FLUXOUTPUT
    RANGE                    = 0 0 0 0
    NAME                     = flux_LW-rad_NORTH.out
    LOCATION                 = LEFT 

  [SELECTION]
    TYPE                     = FLUXOUTPUT
    RANGE                    = 54 0 54 0
    NAME                     = flux_moisture_EAST.out
    LOCATION                 = LEFT 

  [SELECTION]
    TYPE                     = FLUXOUTPUT
    RANGE                    = 54 0 54 0
    NAME                     = flux_rain_normal_EAST.out
    LOCATION                 = LEFT 

  [SELECTION]
    TYPE                     = FLUXOUTPUT
    RANGE                    = 54 0 54 0
    NAME                     = flux_rain_normal_integral_EAST.out
    LOCATION                 = LEFT 

  [SELECTION]
    TYPE                     = FLUXOUTPUT
    RANGE                    = 54 0 54 0
    NAME                     = flux_SW-rad_EAST.out
    LOCATION                 = LEFT 

  [SELECTION]
    TYPE                     = FLUXOUTPUT
    RANGE                    = 54 0 54 0
    NAME                     = flux_LW-rad_EAST.out
    LOCATION                 = LEFT 

  [SELECTION]
    TYPE                     = FLUXOUTPUT
    RANGE                    = 108 0 108 0
    NAME                     = flux_moisture_SOUTH.out
    LOCATION                 = LEFT 

  [SELECTION]
    TYPE                     = FLUXOUTPUT
    RANGE                    = 108 0 108 0
    NAME                     = flux_rain_normal_SOUTH.out
    LOCATION                 = LEFT 

  [SELECTION]
    TYPE                     = FLUXOUTPUT
    RANGE                    = 108 0 108 0
    NAME                     = flux_rain_normal_integral_SOUTH.out
    LOCATION                 = LEFT 

  [SELECTION]
    TYPE                     = FLUXOUTPUT
    RANGE                    = 108 0 108 0
    NAME                     = flux_SW-rad_SOUTH.out
    LOCATION                 = LEFT 

  [SELECTION]
    TYPE                     = FLUXOUTPUT
    RANGE                    = 108 0 108 0
    NAME                     = flux_LW-rad_SOUTH.out
    LOCATION                 = LEFT 

  [SELECTION]
    TYPE                     = FLUXOUTPUT
    RANGE                    = 162 0 162 0
    NAME                     = flux_moisture_WEST.out
    LOCATION                 = LEFT 

  [SELECTION]
    TYPE                     = FLUXOUTPUT
    RANGE                    = 162 0 162 0
    NAME                     = flux_rain_normal_WEST.out
    LOCATION                 = LEFT 

  [SELECTION]
    TYPE                     = FLUXOUTPUT
    RANGE                    = 162 0 162 0
    NAME                     = flux_rain_normal_integral_WEST.out
    LOCATION                 = LEFT 

  [SELECTION]
    TYPE                     = FLUXOUTPUT
    RANGE                    = 162 0 162 0
    NAME                     = flux_SW-rad_WEST.out
    LOCATION                 = LEFT 

  [SELECTION]
    TYPE                     = FLUXOUTPUT
    RANGE                    = 162 0 162 0
    NAME                     = flux_LW-rad_WEST.out
    LOCATION                 = LEFT 


; ******************************************************************************


