D6MARLZ! 006.001

[IDENTIFICATION]
  NAME                     = DE: Calciumsilikatplatte |EN: Calcium Silicate Panel |IT: Pannello in calciosilicato |RU: Пластина из силиката кальция
  AQUISITION_ID            = -1
  PRODUCER                 = DE: Remmers Baustofftechnik GmbH |EN: Remmers Baustofftechnik GmbH |IT: Remmers Baustofftechnik GmbH |RU: Remmers Baustofftechnik
  PRODUCT_ID               = DE: SLP N |EN: SLP N |IT: SLP N |RU: SLP N
  LABORATORY               = DE: IBK-Labor |EN: IBK-Laboratory |IT: Laboratorio IBK |RU: Лаборатория института строительной климатологии
  DATE                     = 13.11.24
  COLOUR                   = #ffff1010
  FLAGS                    = AIR_TIGHT 
  CATEGORY                 = INSULATION BUILDING_BOARDS
  COMMENTS                 = DE: SLP 25 N (25mm), SLP 30 N (30mm), SLP 50 N (50mm), bis 2013 im Handel |EN: SLP 25 N (25mm), SLP 30 N (30mm), SLP 50 N (50mm), in stores until 2013 |IT: SLP 25 N (25mm), SLP 30 N (30mm), SLP 50 N (50mm)
  DBTYPE                   = 1,4,5,6,7,8
  HATCHING                 = 13


[STORAGE_BASE_PARAMETERS]
  RHO                      = 365 kg/m3
  CE                       = 900 J/kgK
  THETA_POR                = 0.951 m3/m3
  THETA_EFF                = 0.95 m3/m3
  THETA_80                 = 0.008 m3/m3


[TRANSPORT_BASE_PARAMETERS]
  LAMBDA                   = 0.064 W/mK
  AW                       = 1.29 kg/m2s05
  MEW                      = 4.6 -
  KLEFF                    = 0 s
  LAMBDA_DESIGN            = 0.0626 W/mK

