D6MARLZ! 006.001

[IDENTIFICATION]
  NAME                     = DE: CLIMA CONTROL NET 160 |EN: CLIMA CONTROL NET 160 |IT: CLIMA CONTROL NET 160
  AQUISITION_ID            = -1
  PRODUCER                 = DE: Rotho Blaas srl |EN: Rotho Blaas srl |IT: Rotho Blaas srl
  LABORATORY               = DE: Eurac Research - Hygrothermal Testing Lab |EN: Eurac Research - Hygrothermal Testing Lab |IT: Eurac Research - Hygrothermal Testing Lab
  DATE                     = 16.07.2021
  SAMPLING_DATE            = 30.11.2020
  COLOUR                   = #ff5020a0
  FLAGS                    = AIR_TIGHT WATER_TIGHT FOILS 
  CATEGORY                 = FOILS
  COMMENTS                 = DE: Materialtyp: Membrane mit variabler Diffusion: PP-Schutzschicht, PA-Folie, Verstärkungsgitter, PP-Schicht - Dicke = 0,5 mm - ;Verwendung in DELPHIN: bei Verwendung als Material muss die Schichtdicke immer 1mm betragen, ab DELPHIN 5.9 wird die Verwendung als Kontaktbedingung statt als Materialschicht empfohlen - ;Materialbeschreibung (Hersteller): CLIMA CONTROL NET 160 verhindert den unkontrollierten Durchgang von warmer und feuchter Luft und die daraus resultierende Gefahr von interstitieller Kondensation. Die Membrane kann sich an die hygrometrischen Bedingungen des Gebäudes anpassen. Sie kann für Dächer und Wände verwendet werden. - ;URL Datenblatt: https://www.rothoblaas.com/products/airtightness-and-waterproofing/membranes |EN: Material Type: Membrane with variable diffusion: PP protective layer, PA film, reinforcing grid, PP layer - Thickness = 0.5 mm - ;Use in DELPHIN: if used as a material the layer thickness must always be 1mm, since DELPHIN 5.9 use as contact condition instead as material layer is recommended - ;Material Description (producer): CLIMA CONTROL NET 160 prevents the uncontrolled passage of warm and moist air and the consequent risk of interstitial condensation. The membrane can adapt to the hygrometric conditions of the building. It can be used  for roofs and walls. - ;URL Datasheet: https://www.rothoblaas.com/products/airtightness-and-waterproofing/membranes |IT: Tipo di Materiale: Membrana a diffusione variabile: strato protettivo in PP, film funzionale in PA, rete di rinforzo, strato in PP - Spessore = 0.5 mm - Utilizzo in DELPHIN: se utilizzato come materiale lo spessore dello strato deve essere di 1 mm, a partire da DELPHIN 5.9 è raccomandato di modellare la membrana come condizione contatto invece che come materiale – Descrizione Materiale (produttore): CLIMA CONTROL NET 160 previene il passaggio incontrollato di calore e umidità e il conseguente rischio di condensa interstiziale. La membrana ha la capacità di adattarsi alle condizioni igrometriche della struttura. Può essere utilizzato su tetti e pareti.   - URL Scheda tecnica: https://www.rothoblaas.com/products/airtightness-and-waterproofing/membranes
  DBTYPE                   = 1,7
  DATA_SHEET_SOURCE        = https://www.rothoblaas.com/products/airtightness-and-waterproofing/membranes
  HATCHING                 = 13


[STORAGE_BASE_PARAMETERS]
  RHO                      = 160 kg/m3
  CE                       = 1800 J/kgK
  THETA_POR                = 0.0025 m3/m3
  THETA_EFF                = 0.0022 m3/m3
  THETA_80                 = 4.85e-05 m3/m3


[TRANSPORT_BASE_PARAMETERS]
  LAMBDA                   = 0.3 W/mK
  MEW                      = 3460 -
  SD                       = 3.46 m


[MOISTURE_STORAGE]
  FUNCTION =              Theta_l(RH)
      0                0.1              0.2              0.3              0.4              0.5              0.6              0.7              0.8              0.85             0.9              0.91             0.92             0.93             0.94             0.95             0.96             0.97             0.98             0.99             0.995            0.999            1                
      0                1.38e-06         3.1e-06          5.3e-06          8.23e-06         1.233e-05        1.844e-05        2.855e-05        4.85e-05         6.808e-05        0.0001062        0.0001186        0.0001339        0.00015325       0.00017848       0.00021278       0.00026211       0.00033909       0.00047606       0.00078787       0.00116299       0.00186817       0.0022           


[MOISTURE_TRANSPORT]
  FUNCTION =              mew(RH)
      0                0.01             0.02             0.03             0.04             0.05             0.06             0.07             0.08             0.09             0.1              0.11             0.12             0.13             0.14             0.15             0.16             0.17             0.18             0.19             0.2              0.21             0.22             0.23             0.24             0.25             0.26             0.27             0.28             0.29             0.3              0.31             0.32             0.33             0.34             0.35             0.36             0.37             0.38             0.39             0.4              0.41             0.42             0.43             0.44             0.45             0.46             0.47             0.48             0.49             0.5              0.51             0.52             0.53             0.54             0.55             0.56             0.57             0.58             0.59             0.6              0.61             0.62             0.63             0.64             0.65             0.66             0.67             0.68             0.69             0.7              0.71             0.72             0.73             0.74             0.75             0.76             0.77             0.78             0.79             0.8              0.81             0.82             0.83             0.84             0.85             0.86             0.87             0.88             0.89             0.9              0.91             0.92             0.93             0.94             0.95             0.96             0.97             0.98             0.99             1                
      3494             3494             3494             3494             3494             3494             3494             3494             3494             3494             3494             3494             3494             3494             3494             3494             3494             3494             3494             3494             3494             3494             3494             3494             3494             3489.57          3485.14          3480.72          3476.3           3471.89          3467.49          3463.09          3458.69          3454.31          3449.92          3445.55          3441.18          3436.81          3432.45          3428.1           3423.75          3419.4           3415.06          3410.73          3406.4           3402.08          3397.77          3393.46          3389.15          3281.93          3081.46          2893.24          2716.51          2550.58          2394.79          2248.51          2111.17          1982.21          1861.13          1747.45          1640.71          1540.5           1446.4           1358.05          1275.1           1197.21          1124.08          1055.42          990.955          930.425          873.593          820.232          772.379          746.648          721.774          697.729          674.485          652.016          630.294          609.297          588.999          569.377          550.409          493.143          420.011          357.724          304.675          259.492          221.01           188.235          160.32           141              141              141              141              141              141              141              141              141              141              


[VAPOR_CONTACT_RESISTANCE]
  FUNCTION =              sd+(rh)
      0                0.2675           0.4165           0.494            0.567            0.629            0.712            0.7945           1                
      3.46             3.46             3.38             2.4              1.44             1.22             0.57             0.35             0.35             
  WEIGHT_FACTOR_POS        = 0.5

