<?xml version="1.0" encoding="UTF-8" ?>
<DelphinProject xmlns="http://www.bauklimatik-dresden.de" xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xmlns:IBK="http://www.bauklimatik-dresden.de/IBK" xsi:schemaLocation="http://www.bauklimatik-dresden.de DelphinProject.xsd" fileVersion="6.1">
	<ProjectInfo created="Tue Oct 09 09:33:18 2012" lastEdited="Di. Mai 18 23:23:35 2021">
		<Comment>&lt;p style=&quot; margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;&quot;&gt;&lt;span style=&quot; font-family:&apos;Courier&apos;; font-size:16pt; font-weight:600; color:#000000;&quot;&gt;Light weight wall&lt;/span&gt;&lt;/p&gt;&#x0A;&lt;p style=&quot; margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;&quot;&gt;&lt;span style=&quot; font-family:&apos;Courier&apos;; font-size:10pt; font-weight:600; color:#000000;&quot;&gt;HAMSTAD: Benchmark 3&lt;/span&gt;&lt;/p&gt;&#x0A;&lt;p style=&quot;-qt-paragraph-type:empty; margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px; font-family:&apos;Courier&apos;; font-size:10pt; font-weight:600; color:#000000;&quot;&gt;&lt;br /&gt;&lt;/p&gt;&#x0A;&lt;p style=&quot; margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;&quot;&gt;&lt;span style=&quot; font-family:&apos;Courier&apos;; font-size:10pt; color:#000000;&quot;&gt;A single layer is analyzed with respect to convective heat and mass transport induced by changing ambient pressure.&lt;/span&gt;&lt;/p&gt;&#x0A;&lt;p style=&quot;-qt-paragraph-type:empty; margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px; font-family:&apos;Courier&apos;; font-size:10pt; color:#000000;&quot;&gt;&lt;br /&gt;&lt;/p&gt;&#x0A;&lt;p style=&quot; margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;&quot;&gt;&lt;span style=&quot; font-family:&apos;Courier&apos;; font-size:10pt; color:#000000;&quot;&gt;This test case evaluates the ability of simulating air flow through the porous medium and its effect on temperature and moisture distribution.&lt;/span&gt;&lt;/p&gt;</Comment>
	</ProjectInfo>

	<!--~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~-->

	<!--Model data, solver settings, general parameters-->
	<Init>
		<SimulationParameter>
			<BalanceEquationModule>BEHeatAirMoisture</BalanceEquationModule>
			<Interval>
				<IBK:Parameter name="Duration" unit="h">2400</IBK:Parameter>
			</Interval>
		</SimulationParameter>
	</Init>

	<!--~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~-->

	<!--List of all materials used in this construction-->
	<Materials>
		<MaterialReference name="Hamstad Benchmark 3 Leight Weight Wall" color="#ff5020a0">${Project Directory}/materials/HamstadBenchmark3LeightWeightWall_16777217.m6</MaterialReference>
	</Materials>

	<!--~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~-->

	<!--Discretization data (grid and sketches)-->
	<Discretization>
		<XSteps unit="m">0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 </XSteps>
	</Discretization>

	<!--~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~-->

	<!--Conditions data, specifies how construction interacts with environment-->
	<Conditions>

		<Interfaces>
			<Interface name="Interface 1" type="Detailed">
				<BCReference>Inside Heat Conduction</BCReference>
				<BCReference>Inside Vapor Diffusion</BCReference>
				<BCReference>Inside Air pressure</BCReference>
			</Interface>
			<Interface name="Interface 2" type="Detailed">
				<BCReference>Outside Heat Conduction</BCReference>
				<BCReference>Outside Vapor Diffusion</BCReference>
				<BCReference>Outside Air pressure</BCReference>
			</Interface>
		</Interfaces>

		<ClimateConditions>

			<ClimateCondition name="Inside Temperature (constant)" type="Temperature" kind="Constant">
				<IBK:Parameter name="ConstantValue" unit="C">20</IBK:Parameter>
			</ClimateCondition>

			<ClimateCondition name="Outside Temperature (constant)" type="Temperature" kind="Constant">
				<IBK:Parameter name="ConstantValue" unit="C">2</IBK:Parameter>
			</ClimateCondition>

			<ClimateCondition name="Inside Relative Humidity (constant)" type="RelativeHumidity" kind="Constant">
				<IBK:Parameter name="ConstantValue" unit="%">70</IBK:Parameter>
			</ClimateCondition>

			<ClimateCondition name="Outside Relative Humidity (constant)" type="RelativeHumidity" kind="Constant">
				<IBK:Parameter name="ConstantValue" unit="%">80</IBK:Parameter>
			</ClimateCondition>

			<ClimateCondition name="Inside Air pressure (data)" type="GasPressure" kind="TabulatedData">
				<Filename>${Project Directory}/climates/HB3_pa_i.ccd</Filename>
				<IBK:Parameter name="ShiftValue" unit="Pa">0</IBK:Parameter>
				<IBK:Flag name="ExtendData">true</IBK:Flag>
			</ClimateCondition>

			<ClimateCondition name="Outside Air pressure (constant)" type="GasPressure" kind="Constant">
				<IBK:Parameter name="ConstantValue" unit="Pa">101325</IBK:Parameter>
			</ClimateCondition>
		</ClimateConditions>

		<BoundaryConditions>

			<BoundaryCondition name="Inside Heat Conduction" type="HeatConduction" kind="Exchange">
				<IBK:Parameter name="ExchangeCoefficient" unit="W/m2K">10</IBK:Parameter>
				<CCReference type="Temperature">Inside Temperature (constant)</CCReference>
			</BoundaryCondition>

			<BoundaryCondition name="Outside Heat Conduction" type="HeatConduction" kind="Exchange">
				<IBK:Parameter name="ExchangeCoefficient" unit="W/m2K">10</IBK:Parameter>
				<CCReference type="Temperature">Outside Temperature (constant)</CCReference>
			</BoundaryCondition>

			<BoundaryCondition name="Inside Vapor Diffusion" type="VaporDiffusion" kind="Exchange">
				<IBK:Parameter name="ExchangeCoefficient" unit="s/m">2e-07</IBK:Parameter>
				<CCReference type="Temperature">Inside Temperature (constant)</CCReference>
				<CCReference type="RelativeHumidity">Inside Relative Humidity (constant)</CCReference>
			</BoundaryCondition>

			<BoundaryCondition name="Outside Vapor Diffusion" type="VaporDiffusion" kind="Exchange">
				<IBK:Parameter name="ExchangeCoefficient" unit="s/m">7.38e-12</IBK:Parameter>
				<CCReference type="Temperature">Outside Temperature (constant)</CCReference>
				<CCReference type="RelativeHumidity">Outside Relative Humidity (constant)</CCReference>
			</BoundaryCondition>

			<BoundaryCondition name="Inside Air pressure" type="AirConvection" kind="Exchange">
				<IBK:Parameter name="ExchangeCoefficient" unit="s/m">1000</IBK:Parameter>
				<CCReference type="Temperature">Inside Temperature (constant)</CCReference>
				<CCReference type="RelativeHumidity">Inside Relative Humidity (constant)</CCReference>
				<CCReference type="GasPressure">Inside Air pressure (data)</CCReference>
			</BoundaryCondition>

			<BoundaryCondition name="Outside Air pressure" type="AirConvection" kind="Exchange">
				<IBK:Parameter name="ExchangeCoefficient" unit="s/m">1000</IBK:Parameter>
				<CCReference type="Temperature">Outside Temperature (constant)</CCReference>
				<CCReference type="RelativeHumidity">Outside Relative Humidity (constant)</CCReference>
				<CCReference type="GasPressure">Outside Air pressure (constant)</CCReference>
			</BoundaryCondition>
		</BoundaryConditions>

		<InitialConditions>

			<InitialCondition name="DEFAULT Initial Temperature" type="Temperature">
				<IBK:Parameter name="Value" unit="C">20</IBK:Parameter>
			</InitialCondition>

			<InitialCondition name="DEFAULT Initial Relative Humidity" type="RelativeHumidity">
				<IBK:Parameter name="Value" unit="%">95</IBK:Parameter>
			</InitialCondition>
		</InitialConditions>
	</Conditions>

	<!--~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~-->

	<!--Contains definitions of output files and schedules for outputs.-->
	<Outputs>
		<!--General parameters-->
		<IBK:Unit name="TimeUnit">d</IBK:Unit>
		<IBK:Flag name="BinaryFormat">false</IBK:Flag>
		<!--List of all Output schedules-->
		<OutputGrids>
			<OutputGrid name="Daily">
				<Interval>
					<IBK:Parameter name="Duration" unit="d">0</IBK:Parameter>
					<IBK:Parameter name="StepSize" unit="d">1</IBK:Parameter>
				</Interval>
			</OutputGrid>
		</OutputGrids>
		<!--List of all Output files-->
		<OutputFiles>
			<OutputFile name="Temp0.05m">
				<Quantity>Temperature</Quantity>
				<TimeType>None</TimeType>
				<SpaceType>Single</SpaceType>
				<OutputGrid>Daily</OutputGrid>
			</OutputFile>
			<OutputFile name="Temp0.10m">
				<Quantity>Temperature</Quantity>
				<TimeType>None</TimeType>
				<SpaceType>Single</SpaceType>
				<OutputGrid>Daily</OutputGrid>
			</OutputFile>
			<OutputFile name="Temp0.15m">
				<Quantity>Temperature</Quantity>
				<TimeType>None</TimeType>
				<SpaceType>Single</SpaceType>
				<OutputGrid>Daily</OutputGrid>
			</OutputFile>
			<OutputFile name="Temp0.17m">
				<Quantity>Temperature</Quantity>
				<TimeType>None</TimeType>
				<SpaceType>Single</SpaceType>
				<OutputGrid>Daily</OutputGrid>
			</OutputFile>
			<OutputFile name="Temp0.19m">
				<Quantity>Temperature</Quantity>
				<TimeType>None</TimeType>
				<SpaceType>Single</SpaceType>
				<OutputGrid>Daily</OutputGrid>
			</OutputFile>
			<OutputFile name="Moist0.05m">
				<Quantity>MoistureMassDensity</Quantity>
				<TimeType>None</TimeType>
				<SpaceType>Single</SpaceType>
				<OutputGrid>Daily</OutputGrid>
			</OutputFile>
			<OutputFile name="Moist0.10m">
				<Quantity>MoistureMassDensity</Quantity>
				<TimeType>None</TimeType>
				<SpaceType>Single</SpaceType>
				<OutputGrid>Daily</OutputGrid>
			</OutputFile>
			<OutputFile name="Moist0.15m">
				<Quantity>MoistureMassDensity</Quantity>
				<TimeType>None</TimeType>
				<SpaceType>Single</SpaceType>
				<OutputGrid>Daily</OutputGrid>
			</OutputFile>
			<OutputFile name="Moist0.17m">
				<Quantity>MoistureMassDensity</Quantity>
				<TimeType>None</TimeType>
				<SpaceType>Single</SpaceType>
				<OutputGrid>Daily</OutputGrid>
			</OutputFile>
			<OutputFile name="Moist0.19m">
				<Quantity>MoistureMassDensity</Quantity>
				<TimeType>None</TimeType>
				<SpaceType>Single</SpaceType>
				<OutputGrid>Daily</OutputGrid>
			</OutputFile>
		</OutputFiles>
	</Outputs>

	<!--~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~-->

	<!--List of all assignments of materials and conditions-->
	<Assignments>

		<Assignment type="Material" location="Element">
			<Reference>Hamstad Benchmark 3 Leight Weight Wall</Reference>
			<Range>0 0 199 0</Range>
		</Assignment>

		<Assignment type="InitialCondition" location="Element">
			<Reference>DEFAULT Initial Temperature</Reference>
			<Range>0 0 199 0</Range>
		</Assignment>

		<Assignment type="InitialCondition" location="Element">
			<Reference>DEFAULT Initial Relative Humidity</Reference>
			<Range>0 0 199 0</Range>
		</Assignment>

		<Assignment type="Output" location="Coordinate">
			<Reference>Temp0.05m</Reference>
			<IBK:Point3D>0.0495 0.5 0.5</IBK:Point3D>
		</Assignment>

		<Assignment type="Output" location="Coordinate">
			<Reference>Temp0.10m</Reference>
			<IBK:Point3D>0.0995 0.5 0.5</IBK:Point3D>
		</Assignment>

		<Assignment type="Output" location="Coordinate">
			<Reference>Temp0.15m</Reference>
			<IBK:Point3D>0.1495 0.5 0.5</IBK:Point3D>
		</Assignment>

		<Assignment type="Output" location="Coordinate">
			<Reference>Temp0.17m</Reference>
			<IBK:Point3D>0.1695 0.5 0.5</IBK:Point3D>
		</Assignment>

		<Assignment type="Output" location="Coordinate">
			<Reference>Temp0.19m</Reference>
			<IBK:Point3D>0.1895 0.5 0.5</IBK:Point3D>
		</Assignment>

		<Assignment type="Output" location="Coordinate">
			<Reference>Moist0.05m</Reference>
			<IBK:Point3D>0.0495 0.5 0.5</IBK:Point3D>
		</Assignment>

		<Assignment type="Output" location="Coordinate">
			<Reference>Moist0.10m</Reference>
			<IBK:Point3D>0.0995 0.5 0.5</IBK:Point3D>
		</Assignment>

		<Assignment type="Output" location="Coordinate">
			<Reference>Moist0.15m</Reference>
			<IBK:Point3D>0.1495 0.5 0.5</IBK:Point3D>
		</Assignment>

		<Assignment type="Output" location="Coordinate">
			<Reference>Moist0.17m</Reference>
			<IBK:Point3D>0.1695 0.5 0.5</IBK:Point3D>
		</Assignment>

		<Assignment type="Output" location="Coordinate">
			<Reference>Moist0.19m</Reference>
			<IBK:Point3D>0.1895 0.5 0.5</IBK:Point3D>
		</Assignment>

		<Assignment type="Interface" location="Left">
			<Reference>Interface 1</Reference>
			<Range>0 0 0 0</Range>
		</Assignment>

		<Assignment type="Interface" location="Right">
			<Reference>Interface 2</Reference>
			<Range>199 0 199 0</Range>
		</Assignment>
	</Assignments>

	<!--~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~-->

</DelphinProject>
