<?xml version="1.0" encoding="UTF-8" ?>
<DelphinProject xmlns="http://www.bauklimatik-dresden.de" xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xmlns:IBK="http://www.bauklimatik-dresden.de/IBK" xsi:schemaLocation="http://www.bauklimatik-dresden.de DelphinProject.xsd" fileVersion="6.5">
	<ProjectInfo created="Mi. Dez. 6 12:43:04 2017" lastEdited="Sa. Apr. 7 19:04:54 2018">
		<Comment>&lt;p style=&quot; margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;&quot;&gt;&lt;span style=&quot; font-family:&apos;Courier&apos;; font-weight:600;&quot;&gt;One-sided freezing of a brick wall&lt;/span&gt;&lt;/p&gt;&#x0A;&lt;p style=&quot;-qt-paragraph-type:empty; margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px; font-family:&apos;Courier&apos;;&quot;&gt;&lt;br /&gt;&lt;/p&gt;&#x0A;&lt;p style=&quot; margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;&quot;&gt;&lt;span style=&quot; font-family:&apos;Courier&apos;;&quot;&gt;A brick wall is moisture-tight on both sides. The left side is cooled down to a constant negative temperature, while the right side maintains a warm temperature. Depending on the initial moisture content in the construction, different temperature and ice content profiles are obtained in the final steady-state.&lt;/span&gt;&lt;/p&gt;&#x0A;&lt;p style=&quot;-qt-paragraph-type:empty; margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px; font-family:&apos;Courier&apos;;&quot;&gt;&lt;br /&gt;&lt;/p&gt;&#x0A;&lt;p style=&quot; margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;&quot;&gt;&lt;span style=&quot; font-family:&apos;Courier&apos;;&quot;&gt;The example illustrates how three different constructions (here with different initial moisture contents) can be modeled in simulated at the same time. The example illustrates correct calculation of freezing point depression and effect of ice content on thermal conductivity.&lt;/span&gt;&lt;/p&gt;&#x0A;&lt;p style=&quot;-qt-paragraph-type:empty; margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px; font-family:&apos;Courier&apos;;&quot;&gt;&lt;br /&gt;&lt;/p&gt;</Comment>
	</ProjectInfo>

	<!--~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~-->

	<!--Model data, solver settings, general parameters-->
	<Init>
		<SimulationParameter>
			<BalanceEquationModule>BEHeatMoisture</BalanceEquationModule>
			<Interval>
				<IBK:Parameter name="Duration" unit="d">10</IBK:Parameter>
			</Interval>
			<IBK:Parameter name="Longitude" unit="Deg">13.4</IBK:Parameter>
			<IBK:Parameter name="Latitude" unit="Deg">51.3</IBK:Parameter>
			<IBK:Flag name="UseKirchhoffPotential">false</IBK:Flag>
			<IBK:Flag name="UseIce">true</IBK:Flag>
			<DefaultInitialCondition name="DefaultTemperature" unit="C">10</DefaultInitialCondition>
		</SimulationParameter>
		<SolverParameter>
			<LESSolver>Band</LESSolver>
			<IBK:Parameter name="AbsTolMoisture" unit="kg">1e-07</IBK:Parameter>
			<IBK:Parameter name="NonlinSolverConvCoeff" unit="---">0.08</IBK:Parameter>
		</SolverParameter>
	</Init>

	<!--~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~-->

	<!--List of all materials used in this construction-->
	<Materials>
		<MaterialReference name="Altbauziegel Schloss Güterfelde (EG_Außenwand 1) [544]" color="#ffa40000" hatchCode="13">${Project Directory}/materials/AltbauziegelSchlossGueterfeldeEGAussenwand1_544.m6</MaterialReference>
	</Materials>

	<!--~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~-->

	<!--Discretization data (grid and sketches)-->
	<Discretization>
		<XSteps unit="m">0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 </XSteps>
		<YSteps unit="m">0.2 0.2 0.2 0.2 0.2 </YSteps>
	</Discretization>

	<!--~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~-->

	<!--Conditions data, specifies how construction interacts with environment-->
	<Conditions>

		<Interfaces>
			<Interface name="Cold side" type="EngineeringIndoor">
				<IBK:Parameter name="CustomIndoorTemperature" unit="C">-10</IBK:Parameter>
				<IBK:Parameter name="CustomIndoorRelativeHumidity" unit="%">80</IBK:Parameter>
				<IBK:Parameter name="CustomIndoorHeatTransferCoefficient" unit="W/m2K">17</IBK:Parameter>
				<IBK:Parameter name="CustomIndoorVaporTransferCoefficient" unit="s/m">0</IBK:Parameter>
				<ClimateTypeIndoor>IndoorUserData</ClimateTypeIndoor>
			</Interface>
			<Interface name="Warm side" type="EngineeringIndoor">
				<IBK:Parameter name="CustomIndoorTemperature" unit="C">20</IBK:Parameter>
				<IBK:Parameter name="CustomIndoorRelativeHumidity" unit="%">50</IBK:Parameter>
				<IBK:Parameter name="CustomIndoorHeatTransferCoefficient" unit="W/m2K">8</IBK:Parameter>
				<IBK:Parameter name="CustomIndoorVaporTransferCoefficient" unit="s/m">0</IBK:Parameter>
				<ClimateTypeIndoor>IndoorUserData</ClimateTypeIndoor>
			</Interface>
		</Interfaces>

		<InitialConditions>

			<InitialCondition name="Moisture saturated" type="RelativeHumidity">
				<IBK:Parameter name="Value" unit="%">100</IBK:Parameter>
			</InitialCondition>

			<InitialCondition name="50 % saturated" type="MoistureContent">
				<IBK:Parameter name="Value" unit="m3/m3">0.232</IBK:Parameter>
			</InitialCondition>
		</InitialConditions>
	</Conditions>

	<!--~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~-->

	<!--Contains definitions of output files and schedules for outputs.-->
	<Outputs>
		<!--General parameters-->
		<IBK:Unit name="TimeUnit">d</IBK:Unit>
		<!--List of all Output schedules-->
		<OutputGrids>
			<OutputGrid name="Felder und Profile">
				<Interval>
					<IBK:Parameter name="Duration" unit="d">5</IBK:Parameter>
					<IBK:Parameter name="StepSize" unit="h">1</IBK:Parameter>
				</Interval>
			</OutputGrid>
			<OutputGrid name="Skalare">
				<Interval>
					<IBK:Parameter name="Duration" unit="a">0</IBK:Parameter>
					<IBK:Parameter name="StepSize" unit="min">10</IBK:Parameter>
				</Interval>
			</OutputGrid>
		</OutputGrids>
		<!--List of all Output files-->
		<OutputFiles>
			<OutputFile name="Profile-Temperature-Saturated">
				<Quantity unit="C">Temperature</Quantity>
				<TimeType>None</TimeType>
				<SpaceType>Single</SpaceType>
				<OutputGrid>Felder und Profile</OutputGrid>
			</OutputFile>
			<OutputFile name="Profile-RelativeHumidity-Saturated">
				<Quantity unit="%">RelativeHumidity</Quantity>
				<TimeType>None</TimeType>
				<SpaceType>Single</SpaceType>
				<OutputGrid>Felder und Profile</OutputGrid>
			</OutputFile>
			<OutputFile name="Profile-LiquidMassDensity-Saturated">
				<Quantity unit="kg/m3">LiquidMassDensity</Quantity>
				<TimeType>None</TimeType>
				<SpaceType>Single</SpaceType>
				<OutputGrid>Felder und Profile</OutputGrid>
			</OutputFile>
			<OutputFile name="Integral-IceMassDensity-Saturated">
				<Quantity unit="kg">IceMassDensity</Quantity>
				<TimeType>None</TimeType>
				<SpaceType>Integral</SpaceType>
				<OutputGrid>Skalare</OutputGrid>
			</OutputFile>
			<OutputFile name="Profile-Temperature-MediumWet">
				<Quantity unit="C">Temperature</Quantity>
				<TimeType>None</TimeType>
				<SpaceType>Single</SpaceType>
				<OutputGrid>Felder und Profile</OutputGrid>
			</OutputFile>
			<OutputFile name="Profile-RelativeHumidity-MediumWet">
				<Quantity unit="%">RelativeHumidity</Quantity>
				<TimeType>None</TimeType>
				<SpaceType>Single</SpaceType>
				<OutputGrid>Felder und Profile</OutputGrid>
			</OutputFile>
			<OutputFile name="Profile-LiquidMassDensity-MediumWet">
				<Quantity unit="kg/m3">LiquidMassDensity</Quantity>
				<TimeType>None</TimeType>
				<SpaceType>Single</SpaceType>
				<OutputGrid>Felder und Profile</OutputGrid>
			</OutputFile>
			<OutputFile name="Integral-IceMassDensity-MediumWet">
				<Quantity unit="kg">IceMassDensity</Quantity>
				<TimeType>None</TimeType>
				<SpaceType>Integral</SpaceType>
				<OutputGrid>Skalare</OutputGrid>
			</OutputFile>
			<OutputFile name="Profile-Temperature-Dry">
				<Quantity unit="C">Temperature</Quantity>
				<TimeType>None</TimeType>
				<SpaceType>Single</SpaceType>
				<OutputGrid>Felder und Profile</OutputGrid>
			</OutputFile>
			<OutputFile name="Profile-RelativeHumidity-Dry">
				<Quantity unit="%">RelativeHumidity</Quantity>
				<TimeType>None</TimeType>
				<SpaceType>Single</SpaceType>
				<OutputGrid>Felder und Profile</OutputGrid>
			</OutputFile>
			<OutputFile name="Profile-LiquidMassDensity-Dry">
				<Quantity unit="kg/m3">LiquidMassDensity</Quantity>
				<TimeType>None</TimeType>
				<SpaceType>Single</SpaceType>
				<OutputGrid>Felder und Profile</OutputGrid>
			</OutputFile>
			<OutputFile name="Integral-IceMassDensity-Dry">
				<Quantity unit="kg">IceMassDensity</Quantity>
				<TimeType>None</TimeType>
				<SpaceType>Integral</SpaceType>
				<OutputGrid>Skalare</OutputGrid>
			</OutputFile>
			<OutputFile name="Profile-IceMassDensity-Saturated">
				<Quantity unit="kg/m3">IceMassDensity</Quantity>
				<TimeType>None</TimeType>
				<SpaceType>Single</SpaceType>
				<OutputGrid>Felder und Profile</OutputGrid>
			</OutputFile>
			<OutputFile name="Profile-IceMassDensity-MediumWet">
				<Quantity unit="kg/m3">IceMassDensity</Quantity>
				<TimeType>None</TimeType>
				<SpaceType>Single</SpaceType>
				<OutputGrid>Felder und Profile</OutputGrid>
			</OutputFile>
			<OutputFile name="Profile-IceMassDensity-Dry">
				<Quantity unit="kg/m3">IceMassDensity</Quantity>
				<TimeType>None</TimeType>
				<SpaceType>Single</SpaceType>
				<OutputGrid>Felder und Profile</OutputGrid>
			</OutputFile>
			<OutputFile name="Profile-MoistureMassDensity-Saturated">
				<Quantity unit="kg/m3">MoistureMassDensity</Quantity>
				<TimeType>None</TimeType>
				<SpaceType>Single</SpaceType>
				<OutputGrid>Felder und Profile</OutputGrid>
			</OutputFile>
			<OutputFile name="Profile-MoistureMassDensity-MediumWet">
				<Quantity unit="kg/m3">MoistureMassDensity</Quantity>
				<TimeType>None</TimeType>
				<SpaceType>Single</SpaceType>
				<OutputGrid>Felder und Profile</OutputGrid>
			</OutputFile>
			<OutputFile name="Profile-MoistureMassDensity-Dry">
				<Quantity unit="kg/m3">MoistureMassDensity</Quantity>
				<TimeType>None</TimeType>
				<SpaceType>Single</SpaceType>
				<OutputGrid>Felder und Profile</OutputGrid>
			</OutputFile>
			<OutputFile name="Capillary pressure-MediumWet">
				<Quantity unit="Pa">CapillaryPressure</Quantity>
				<TimeType>None</TimeType>
				<SpaceType>Single</SpaceType>
				<OutputGrid>Felder und Profile</OutputGrid>
			</OutputFile>
			<OutputFile name="VaporPressure-MediumWet">
				<Quantity unit="Pa">VaporPressure</Quantity>
				<TimeType>None</TimeType>
				<SpaceType>Single</SpaceType>
				<OutputGrid>Felder und Profile</OutputGrid>
			</OutputFile>
			<OutputFile name="Profile-Vapor flux densities-MediumWet">
				<Quantity unit="kg/m2s">FluxVaporDiffusion</Quantity>
				<TimeType>None</TimeType>
				<SpaceType>Single</SpaceType>
				<OutputGrid>Felder und Profile</OutputGrid>
			</OutputFile>
			<OutputFile name="Profile-Liquid flux densities-MediumWet">
				<Quantity unit="kg/m2s">FluxLiquidConvection</Quantity>
				<TimeType>None</TimeType>
				<SpaceType>Single</SpaceType>
				<OutputGrid>Felder und Profile</OutputGrid>
			</OutputFile>
		</OutputFiles>
	</Outputs>

	<!--~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~-->

	<!--List of all assignments of materials and conditions-->
	<Assignments>

		<Assignment type="Material" location="Element">
			<Reference>Altbauziegel Schloss Güterfelde (EG_Außenwand 1) [544]</Reference>
			<Range>0 0 99 4</Range>
		</Assignment>

		<Assignment type="Interface" location="Left">
			<Reference>Cold side</Reference>
			<Range>0 0 0 4</Range>
		</Assignment>

		<Assignment type="Interface" location="Right">
			<Reference>Warm side</Reference>
			<Range>99 0 99 4</Range>
		</Assignment>

		<Assignment type="Material" location="Element">
			<Reference>VOID</Reference>
			<Range>0 3 99 3</Range>
		</Assignment>

		<Assignment type="Material" location="Element">
			<Reference>VOID</Reference>
			<Range>0 1 99 1</Range>
		</Assignment>

		<Assignment type="InitialCondition" location="Element">
			<Reference>Moisture saturated</Reference>
			<Range>0 4 99 4</Range>
		</Assignment>

		<Assignment type="InitialCondition" location="Element">
			<Reference>50 % saturated</Reference>
			<Range>0 2 99 2</Range>
		</Assignment>

		<Assignment type="Output" location="Element">
			<Reference>Profile-Temperature-Dry</Reference>
			<Range>0 0 99 0</Range>
		</Assignment>

		<Assignment type="Output" location="Element">
			<Reference>Profile-RelativeHumidity-Dry</Reference>
			<Range>0 0 99 0</Range>
		</Assignment>

		<Assignment type="Output" location="Element">
			<Reference>Profile-LiquidMassDensity-Dry</Reference>
			<Range>0 0 99 0</Range>
		</Assignment>

		<Assignment type="Output" location="Element">
			<Reference>Integral-IceMassDensity-Dry</Reference>
			<Range>0 0 99 0</Range>
		</Assignment>

		<Assignment type="Output" location="Element">
			<Reference>Profile-Temperature-MediumWet</Reference>
			<Range>0 2 99 2</Range>
		</Assignment>

		<Assignment type="Output" location="Element">
			<Reference>Profile-RelativeHumidity-MediumWet</Reference>
			<Range>0 2 99 2</Range>
		</Assignment>

		<Assignment type="Output" location="Element">
			<Reference>Profile-LiquidMassDensity-MediumWet</Reference>
			<Range>0 2 99 2</Range>
		</Assignment>

		<Assignment type="Output" location="Element">
			<Reference>Integral-IceMassDensity-MediumWet</Reference>
			<Range>0 2 99 2</Range>
		</Assignment>

		<Assignment type="Output" location="Element">
			<Reference>Profile-Temperature-Saturated</Reference>
			<Range>0 4 99 4</Range>
		</Assignment>

		<Assignment type="Output" location="Element">
			<Reference>Profile-RelativeHumidity-Saturated</Reference>
			<Range>0 4 99 4</Range>
		</Assignment>

		<Assignment type="Output" location="Element">
			<Reference>Profile-LiquidMassDensity-Saturated</Reference>
			<Range>0 4 99 4</Range>
		</Assignment>

		<Assignment type="Output" location="Element">
			<Reference>Integral-IceMassDensity-Saturated</Reference>
			<Range>0 4 99 4</Range>
		</Assignment>

		<Assignment type="Output" location="Element">
			<Reference>Profile-IceMassDensity-Saturated</Reference>
			<Range>0 4 99 4</Range>
		</Assignment>

		<Assignment type="Output" location="Element">
			<Reference>Profile-IceMassDensity-MediumWet</Reference>
			<Range>0 2 99 2</Range>
		</Assignment>

		<Assignment type="Output" location="Element">
			<Reference>Profile-IceMassDensity-Dry</Reference>
			<Range>0 0 99 0</Range>
		</Assignment>

		<Assignment type="Output" location="Element">
			<Reference>Profile-MoistureMassDensity-Saturated</Reference>
			<Range>0 4 99 4</Range>
		</Assignment>

		<Assignment type="Output" location="Element">
			<Reference>Profile-MoistureMassDensity-MediumWet</Reference>
			<Range>0 2 99 2</Range>
		</Assignment>

		<Assignment type="Output" location="Element">
			<Reference>Profile-MoistureMassDensity-Dry</Reference>
			<Range>0 0 99 0</Range>
		</Assignment>

		<Assignment type="Output" location="Element">
			<Reference>Capillary pressure-MediumWet</Reference>
			<Range>0 2 99 2</Range>
		</Assignment>

		<Assignment type="Output" location="Element">
			<Reference>VaporPressure-MediumWet</Reference>
			<Range>0 2 99 2</Range>
		</Assignment>

		<Assignment type="Output" location="Element">
			<Reference>Profile-Vapor flux densities-MediumWet</Reference>
			<Range>0 2 99 2</Range>
		</Assignment>

		<Assignment type="Output" location="Element">
			<Reference>Profile-Liquid flux densities-MediumWet</Reference>
			<Range>0 2 99 2</Range>
		</Assignment>
	</Assignments>

	<!--~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~-->

</DelphinProject>
