<?xml version="1.0" encoding="UTF-8" ?>
<DelphinProject xmlns="http://www.bauklimatik-dresden.de" xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xmlns:IBK="http://www.bauklimatik-dresden.de/IBK" xsi:schemaLocation="http://www.bauklimatik-dresden.de DelphinProject.xsd" fileVersion="6.1">
	<ProjectInfo created="Mon Oct 08 16:05:55 2012" lastEdited="Di. Mai 18 19:15:13 2021">
		<Comment>&lt;p style=&quot; margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;&quot;&gt;&lt;span style=&quot; font-family:&apos;Courier&apos;; font-size:16pt; font-weight:600;&quot;&gt;Insulated roof&lt;/span&gt;&lt;/p&gt;&#x0A;&lt;p style=&quot; margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;&quot;&gt;&lt;span style=&quot; font-family:&apos;Courier&apos;; font-size:10pt; font-weight:600;&quot;&gt;HAMSTAD: Benchmark 1&lt;/span&gt;&lt;/p&gt;&#x0A;&lt;p style=&quot;-qt-paragraph-type:empty; margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px; font-family:&apos;Courier&apos;; font-size:10pt; font-weight:600;&quot;&gt;&lt;br /&gt;&lt;/p&gt;&#x0A;&lt;p style=&quot; margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;&quot;&gt;&lt;span style=&quot; font-family:&apos;Courier&apos;; font-size:10pt; color:#000000;&quot;&gt;An insulated roof structure is analysed in one dimension. The thermal insulation is facing the interior and there is a moisture barrier facing the exterior. The structure is perfectly airtight.&lt;/span&gt;&lt;/p&gt;&#x0A;&lt;p style=&quot;-qt-paragraph-type:empty; margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px; font-family:&apos;Courier&apos;; font-size:10pt; color:#000000;&quot;&gt;&lt;br /&gt;&lt;/p&gt;&#x0A;&lt;p style=&quot; margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;&quot;&gt;&lt;span style=&quot; font-family:&apos;Courier&apos;; font-size:10pt; color:#000000;&quot;&gt;This test case evaluates the correct calculation of transient profiles using realistic ambient climate data.&lt;/span&gt;&lt;/p&gt;</Comment>
	</ProjectInfo>

	<!--~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~-->

	<!--Model data, solver settings, general parameters-->
	<Init>
		<SimulationParameter>
			<BalanceEquationModule>BEHeatMoisture</BalanceEquationModule>
			<Interval>
				<IBK:Parameter name="Duration" unit="a">5</IBK:Parameter>
			</Interval>
		</SimulationParameter>
		<SolverParameter>
			<IBK:Parameter name="MinTimeStep" unit="s">1e-05</IBK:Parameter>
		</SolverParameter>
	</Init>

	<!--~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~-->

	<!--List of all materials used in this construction-->
	<Materials>
		<MaterialReference name="Hamstad Benchmark 1 Load bearing material" color="#ff404060">${Project Directory}/materials/HamstadBenchmark1Loadbearingmaterial_16777217.m6</MaterialReference>
		<MaterialReference name="Hamstad Benchmark 1 Insulation Material" color="#ff409020">${Project Directory}/materials/HamstadBenchmark1InsulationMaterial_16777218.m6</MaterialReference>
	</Materials>

	<!--~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~-->

	<!--Discretization data (grid and sketches)-->
	<Discretization>
		<XSteps unit="m">1 </XSteps>
		<YSteps unit="m">0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 0.001 </YSteps>
	</Discretization>

	<!--~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~-->

	<!--Conditions data, specifies how construction interacts with environment-->
	<Conditions>

		<Interfaces>
			<Interface name="Interface 1" type="Detailed">
				<BCReference>Outside Heat Conduction</BCReference>
			</Interface>
			<Interface name="Interface 2" type="Detailed">
				<BCReference>Inside Heat Conduction</BCReference>
				<BCReference>Inside Vapour Diffusion</BCReference>
			</Interface>
		</Interfaces>

		<ClimateConditions>

			<ClimateCondition name="Inside Temperatures (constant)" type="Temperature" kind="Constant">
				<IBK:Parameter name="ConstantValue" unit="C">20</IBK:Parameter>
			</ClimateCondition>

			<ClimateCondition name="Outside Temperature (data points)" type="Temperature" kind="TabulatedData">
				<Filename>${Project Directory}/climates/HB1_Teq_e.ccd</Filename>
				<IBK:Parameter name="ShiftValue" unit="K">0</IBK:Parameter>
			</ClimateCondition>

			<ClimateCondition name="Inside Water Vapour Pressure" type="VaporPressure" kind="TabulatedData">
				<Filename>${Project Directory}/climates/HB1_pa_i.ccd</Filename>
				<IBK:Parameter name="ShiftValue" unit="Pa">0</IBK:Parameter>
			</ClimateCondition>

			<ClimateCondition name="Outside Water Vapour Pressure" type="VaporPressure" kind="TabulatedData">
				<Filename>${Project Directory}/climates/HB1_pa_e.ccd</Filename>
				<IBK:Parameter name="ShiftValue" unit="Pa">0</IBK:Parameter>
			</ClimateCondition>
		</ClimateConditions>

		<BoundaryConditions>

			<BoundaryCondition name="Inside Heat Conduction" type="HeatConduction" kind="Exchange">
				<IBK:Parameter name="ExchangeCoefficient" unit="W/m2K">7</IBK:Parameter>
				<CCReference type="Temperature">Inside Temperatures (constant)</CCReference>
			</BoundaryCondition>

			<BoundaryCondition name="Outside Heat Conduction" type="HeatConduction" kind="Exchange">
				<IBK:Parameter name="ExchangeCoefficient" unit="W/m2K">25</IBK:Parameter>
				<CCReference type="Temperature">Outside Temperature (data points)</CCReference>
			</BoundaryCondition>

			<BoundaryCondition name="Inside Vapour Diffusion" type="VaporDiffusion" kind="Exchange">
				<IBK:Parameter name="ExchangeCoefficient" unit="s/m">2e-08</IBK:Parameter>
				<IBK:Flag name="UseVaporPressure">true</IBK:Flag>
				<CCReference type="Temperature">Inside Temperatures (constant)</CCReference>
				<CCReference type="VaporPressure">Inside Water Vapour Pressure</CCReference>
			</BoundaryCondition>
		</BoundaryConditions>

		<InitialConditions>

			<InitialCondition name="Temperatur" type="Temperature">
				<IBK:Parameter name="Value" unit="C">10</IBK:Parameter>
			</InitialCondition>

			<InitialCondition name="Wassergehalt_MaterialA" type="MoistureMass">
				<IBK:Parameter name="Value" unit="kg/m3">145</IBK:Parameter>
			</InitialCondition>

			<InitialCondition name="Wassergehalt_MaterialB" type="MoistureMass">
				<IBK:Parameter name="Value" unit="kg/m3">0.065</IBK:Parameter>
			</InitialCondition>
		</InitialConditions>
	</Conditions>

	<!--~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~-->

	<!--Contains definitions of output files and schedules for outputs.-->
	<Outputs>
		<!--General parameters-->
		<IBK:Unit name="TimeUnit">d</IBK:Unit>
		<IBK:Flag name="BinaryFormat">false</IBK:Flag>
		<!--List of all Output schedules-->
		<OutputGrids>
			<OutputGrid name="Hourly">
				<Interval>
					<IBK:Parameter name="Duration" unit="a">1</IBK:Parameter>
					<IBK:Parameter name="StepSize" unit="h">1</IBK:Parameter>
				</Interval>
				<Interval>
					<IBK:Parameter name="Duration" unit="a">3</IBK:Parameter>
					<IBK:Parameter name="StepSize" unit="a">3</IBK:Parameter>
				</Interval>
				<Interval>
					<IBK:Parameter name="Duration" unit="d">0</IBK:Parameter>
					<IBK:Parameter name="StepSize" unit="h">1</IBK:Parameter>
				</Interval>
			</OutputGrid>
		</OutputGrids>
		<!--List of all Output files-->
		<OutputFiles>
			<OutputFile name="HeatFluxInside">
				<Quantity>FluxHeatConduction</Quantity>
				<TimeType>None</TimeType>
				<SpaceType>Single</SpaceType>
				<OutputGrid>Hourly</OutputGrid>
			</OutputFile>
			<OutputFile name="MoistMaterialA">
				<Quantity>MoistureMassDensity</Quantity>
				<TimeType>None</TimeType>
				<SpaceType>Integral</SpaceType>
				<OutputGrid>Hourly</OutputGrid>
			</OutputFile>
			<OutputFile name="MoistMaterialB">
				<Quantity>MoistureMassDensity</Quantity>
				<TimeType>None</TimeType>
				<SpaceType>Integral</SpaceType>
				<OutputGrid>Hourly</OutputGrid>
			</OutputFile>
			<OutputFile name="Moist0.0167m">
				<Quantity>MoistureMassDensity</Quantity>
				<TimeType>None</TimeType>
				<SpaceType>Single</SpaceType>
				<OutputGrid>Hourly</OutputGrid>
			</OutputFile>
			<OutputFile name="Moist0.05m">
				<Quantity>MoistureMassDensity</Quantity>
				<TimeType>None</TimeType>
				<SpaceType>Single</SpaceType>
				<OutputGrid>Hourly</OutputGrid>
			</OutputFile>
			<OutputFile name="Moist0.0834">
				<Quantity>MoistureMassDensity</Quantity>
				<TimeType>None</TimeType>
				<SpaceType>Single</SpaceType>
				<OutputGrid>Hourly</OutputGrid>
			</OutputFile>
			<OutputFile name="Moist0.125">
				<Quantity>MoistureMassDensity</Quantity>
				<TimeType>None</TimeType>
				<SpaceType>Single</SpaceType>
				<OutputGrid>Hourly</OutputGrid>
			</OutputFile>
		</OutputFiles>
	</Outputs>

	<!--~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~-->

	<!--List of all assignments of materials and conditions-->
	<Assignments>

		<Assignment type="Material" location="Element">
			<Reference>Hamstad Benchmark 1 Load bearing material</Reference>
			<Range>0 50 0 149</Range>
		</Assignment>

		<Assignment type="Material" location="Element">
			<Reference>Hamstad Benchmark 1 Insulation Material</Reference>
			<Range>0 0 0 49</Range>
		</Assignment>

		<Assignment type="InitialCondition" location="Element">
			<Reference>Temperatur</Reference>
			<Range>0 0 0 149</Range>
		</Assignment>

		<Assignment type="InitialCondition" location="Element">
			<Reference>Wassergehalt_MaterialA</Reference>
			<Range>0 50 0 149</Range>
		</Assignment>

		<Assignment type="InitialCondition" location="Element">
			<Reference>Wassergehalt_MaterialB</Reference>
			<Range>0 0 0 49</Range>
		</Assignment>

		<Assignment type="Output" location="Element">
			<Reference>MoistMaterialA</Reference>
			<Range>0 50 0 149</Range>
		</Assignment>

		<Assignment type="Output" location="Element">
			<Reference>MoistMaterialB</Reference>
			<Range>0 0 0 49</Range>
		</Assignment>

		<Assignment type="Output" location="Bottom">
			<Reference>HeatFluxInside</Reference>
			<Range>0 0 0 0</Range>
		</Assignment>

		<Assignment type="Interface" location="Top">
			<Reference>Interface 1</Reference>
			<Range>0 149 0 149</Range>
		</Assignment>

		<Assignment type="Interface" location="Bottom">
			<Reference>Interface 2</Reference>
			<Range>0 0 0 0</Range>
		</Assignment>
	</Assignments>

	<!--~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~-->

</DelphinProject>
